COMMANDO LAV-300 F

CREW: 3 (Driver, Commander & Gunner) + 2 Passengers
CONFIGURATION: 6 x 6
LENGTH: 6.40 m
WIDTH: 2.54 m
HEIGHT (TURRET): 2.53 m
       (HULL): 1.98 m
WEIGHT (EMPTY): 11 818 kg
       (LOADED): 13 318 kg
CARGO CAPACITY: 2000 kg
MAX. TOWED WEIGHT: 2000 kg
GROUND CLEARANCE (AXLES): 0.38 m
                 (HULL): 0.53 m
TURNING RADIUS: 10.00 m
MAX. ROAD SPEED: 92.00 km/h
MAX. CROSS-COUNTRY SPEED: 30.00 km/h
MAX. WATER SPEED: 5.00 km/h
FORDING DEPTH: Amphibious
GRADIENT: 60%
SIDE SLOPE: 30%
VERTICAL OBSTACLE: 0.61 m
TRENCH: 0.5 m
ARMOUR CLASS: 100 all around
ARMAMENT: M2HB .50 cal HMG, Main 
          M240 7.62 mm MMG, Co-Axial
MAXIMUM RATE OF TURRET, POWER TRAVERSE: 25ø/ second
MAXIMUM RATE OF TURRET, MANUAL ELEVATION: 6ø/ second
MAIN & CO-AXIAL, GUN ELEVATION/ DEPRESSION: +55ø/ -10ø Manual
TURRET TRAVERSE: 360ø
AMMUNITION: 210/ 1050 .50 cal (Ready/ Stored)
            200/ 1200 7.62 mm
            4 Anti-Personal, 4 Smoke/ 12 AP, 12 Smoke
SMOKE LAYING EQUIPMENT: 2 x 4 Tube M257 Smoke Launcher
EQUIPMENT: See Attached Sheets
NOTES: 
- The vehicle has a 500 000 candlepower spotlight mounted co-
  axially with the main gun, that will illuminate up to 1.5 kms
  away.  
- The turret is a 1 man turret.
- Winch (Max 9072 kg Tow Limit, 45 m x 12.7 mm Tow Cable).  
- Vehicle is NBCW Proof and Amphibious.
- Tires are 14.50" x 21" Tubeless Tires, with Hutchinson Run Flat
  Insert, which are good for 50 Kms once flat.
- Fusion Engine can be removed and replaced in 1 hour, with
  proper tools and crane.

AMMUNITION:

 M2HB HMG .50 cal

  ********************* -  
  ********************* -  
  ********************* -
  ********************* -
  ********************* -
  ********************* ---

 Short Burst = 10 rds, Medium = 20 rds, Long = 30 rds.

 M240 7.62 mm Co-Axial Machine Gun

  ********************************* - 
  ********************************* - 
  ********************************* - 
  ********************************* - 
  ********************************* - 
  ********************************* - 
  ********************************* --- 
 
  AP, AP, AP, AP, API-T, API-T

 Short Burst = 6 rds, Medium = 12 rds, Long = 18 rds

 M257 66 mm Smoke/ Anti-Personnel Grenade Launchers

  Left       Right

  SA/AS -    SA/AS -
  SA/AS -    SA/AS -
  SA/AS -    SA/AS -
  SA/AS -    SA/AS ---

  A = Anti-Personal   S = Smoke

 Fired in volleys of 4 or 8 at a time.
 When firing mark off one side of the slash.

 Armbrust 300

 * - * - * - * ---