M997/ M997A1 HMMWV 4-Litter "Maxi" Ambulance

CREW: 2 (Driver & Medic) + 8 Ambulatory or 4 Litter Patients or
      Combination of litter and ambulatory patients.
CONFIGURATION: 4 x 4
LENGTH: 4.57 m
WIDTH: 2.15 m
HEIGHT: 2.57 m
WEIGHT (M997; EMPTY): 2996 kg
       (M997A1; EMPTY): 2996 kg
       (M997; LOADED): 4131 kg
       (M997A1; LOADED): 4213 kg
PAYLOAD (M997): 1135 kg
        (M997A1): 1217 kg
MAX. TOWED WEIGHT: 1500 kg
GROUND CLEARANCE (AXLES): 0.41 m
                 (CHASSIS): 0.61 m
TURNING RADIUS: 7.32 m
MAX. ROAD SPEED: 105.00 km/h
AVERAGE ROAD SPEED: 50 km/h
MAX. CROSS-COUNTRY SPEED: 40.00 km/h
ACCELERATION (0 - 48 km/h): 7 seconds
             (0 - 80 km/h): 20 seconds
FORDING DEPTH (W/0 PREPARATION): 0.76 m
              (W/ PREPARATION): 1.50 m
GRADIENT: 60%
SIDE SLOPE: 40%
VERTICAL OBSTACLE: 0.56 m
ARMOUR CLASS (FRONT): 10 (REAR): 7 (SIDES): 7 (TOP): 7
             (BOTTOM): 7
WINDOW HIT: 9+ (Front)
ARMAMENT: None
ARMAMENT TRAVERSE: None
AMMUNITION: None
EQUIPMENT: See Attached Sheets
NOTES: 
- The vehicles are equipped with basic armour and used to
  transport patients from the battlefield.
- Ambulance is provided with NBCW protection, heating, Air-
  Conditioning and power generation.
- A1 Improvements include higher cargo payload, rear springs,
  spring seats, frame crossmembers and shocks were modified.
- Tires are Goodyear 37x12.5 R16.5, with runflat inserts.
  Once one or more tires are flat, the tires can be run for up to
  50 km at 30 km/h.  However, the tire may be ruined beyond
  repair.
- Fusion Engine can be removed and replaced in 1/2 an hour, with
  proper tools and crane.
- Payload includes crew, patients, personal gear, BII (Basic
  Issue Items), special kits & equipment and trailer tongue
  weight.
