HMMVW High Mobility Trailer (HMT), M1101 HMT-L, M1102 HMT-H

CONFIGURATION: 2 Wheeled Trailer
LENGTH: 3.35 m 
WIDTH: 2.22 m
HEIGHT (HMT-L): 1.33 m
       (HMT-H): 1.33 m
WEIGHT (HMT-L; EMPTY): 618 kg
       (HMT-H; EMPTY): 618 kg
       (HMT-L; LOADED): 1542 kg
       (HMT-H LOADED): 1905 kg
PAYLOAD (HMT-L): 927 kg
        (HMT-H): 1291 kg
GROUND CLEARANCE (AXLES): 0.41 m
DECK LENGTH: 2.31 m
DECK WIDTH: 2.04 m
DECK WIDTH (BETWEEN FENDERS): 1.40 m
NOTES: 
- Trailer has been designed for the use on the HMMWV series of
  vehicles, but others can tow the trailer.
- 3 Jacks to support trailer when unhooked from HMMWV.
- Tires are Goodyear 37x12.5 R16.5 (which are the same as the
  tires and rims mounted on any HMMWV variant), with runflat
  inserts.  Once one or more tires are flat, the tires can be run
  for up to 50 km at 30 km/h.  However, the tire may be ruined
  beyond repair.
