COMMANDO V-150 SF COMMAND & CONTROL

CREW: 3 (Driver, Commander, Gunner) + 4 Staff Members
CONFIGURATION: 4 x 4
LENGTH: 6.14 m
WIDTH: 2.26 m
HEIGHT: 2.81 m
WEIGHT (EMPTY): 8054 kg
       (LOADED): 9072 kg
CARGO CAPACITY: 2000 kg
MAX. TOWED WEIGHT: 2000 kg
GROUND CLEARANCE (AXLES): 0.38 m
                 (HULL): 0.65 m
TURNING RADIUS: 8.50 m
MAX. ROAD SPEED: 88.50 km/h
MAX. CROSS-COUNTRY SPEED: 30.00 km/h
MAX. WATER SPEED: 5.00 km/h
FORDING DEPTH: Amphibious
GRADIENT: 60%
SIDE SLOPE: 30%
VERTICAL OBSTACLE: 0.91 m
TRENCH: 0.5 m
ARMOUR CLASS: 100 all around
ARMAMENT: M240D 7.62 mm Machine Gun, Pintle, Anti-Aircraft
       or M2HB .50 cal Heavy Machine Gun, pintle, Anti-Aircraft   
       or Mk 19 Mod 3 40 mm Grenade Launcher
AMMUNITION: 200/ 1000 7.62 mm, Anti-Aircraft
         or 105/ 945 .50 cal, Anti-Aircraft 
         or 50/ 300 40 mm High Velocity
            4 Anti-Personal, 4 Smoke/ 12 AP, 12 Smoke
SMOKE LAYING EQUIPMENT: 2 x 4 Tube M257 Smoke Launcher
EQUIPMENT: See Attached Sheets
NOTES: 
- Externally the vehicle looks very simular to the mortar and
  ambulance Commandos, but doesn't have the opening roof hatches.
  The roof hatch is a circular roof hatch which opens to the
  rear.
- Internally the vehicle has a mapboard, fold down table, and 2
  extra radios.  Other communications equipment maybe added as
  needed, ie. satellite communications gear.  All this extra
  equipment is in place of the passenger compartment.
- Full vehicle air conditioning is provided for crew comfort.
- Winch (Max 4536 kg Tow Limit, 48.76 m x 9.5 mm Tow Cable).  
- Vehicle is NBCW Proof and Amphibious.
- Tires are 14.50" x 21" Tubeless Tires, with Hutchinson Run Flat
  Insert which are good for 50 Kms once flat.
- Fusion Engine can be removed and replaced in 1 hour, with
  proper tools and crane.

AMMUNITION:

 M240D 7.62 mm Anti-Aircraft Machine Gun

  ********************************* - 
  ********************************* - 
  ********************************* - 
  ********************************* - 
  ********************************* - 
  ********************************* --- 

     AP, AP, AP, AP, API-T, API-T

 Short Burst = 6 rds, Medium = 12 rds, Long = 18 rds

or

 M2HB HMG .50 cal

  ************ -
  ************ -
  ************ -
  ************ -
  ************ -
  ************ -
  ************ -
  ************ -
  ************ -
  ************ ---

 Short Burst = 10 rds, Medium = 20 rds, Long = 30 rds.

or

 Mk 19 Mod 3 40 mm GL

  HHW, HHW, HHW, HHW, HHW, HHW, HHW, HHW, HHW, HHW, HHW, HHW,
  HHW, HHW, HHW, HH -

  HHW, HHW, HHW, HHW, HHW, HHW, HHW, HHW, HHW, HHW, HHW, HHW,
  HHW, HHW, HHW, HH -

  HHW, HHW, HHW, HHW, HHW, HHW, HHW, HHW, HHW, HHW, HHW, HHW,
  HHW, HHW, HHW, HH -

  HHW, HHW, HHW, HHW, HHW, HHW, HHW, HHW, HHW, HHW, HHW, HHW,
  HHW, HHW, HHW, HH -

  HHW, HHW, HHW, HHW, HHW, HHW, HHW, HHW, HHW, HHW, HHW, HHW,
  HHW, HHW, HHW, HH -

  HHW, HHW, HHW, HHW, HHW, HHW, HHW, HHW, HHW, HHW, HHW, HHW,
  HHW, HHW, HHW, HH -

  HHW, HHW, HHW, HHW, HHW, HHW, HHW, HHW, HHW, HHW, HHW, HHW,
  HHW, HHW, HHW, HH ---

     H = High Explosive Dual Purpose  W = White Phosphorus

 Short Burst = 3 rds, Medium = 6 rds, Long = 9 rds

 M257 66 mm Smoke/ Anti-Personnel Grenade Launchers

  Left       Right

  SA/AS -    SA/AS -
  SA/AS -    SA/AS -
  SA/AS -    SA/AS -
  SA/AS -    SA/AS ---

  A = Anti-Personal   S = Smoke

 Fired in volleys of 4 or 8 at a time.
 When firing mark off one side of the slash.

 Armbrust 300

 * - * - * - * ---