COMMANDO LAV-300 F WFSV (Wheeled Fire Support Vehicle)

CREW: 3 (Driver, Commander/ Loader & Gunner)
CONFIGURATION: 6 x 6
LENGTH: 6.40 m
WIDTH: 2.54 m
HEIGHT (TURRET): 2.69 m
       (HULL): 1.98 m
WEIGHT (EMPTY): 12 700 kg
       (LOADED): 14 200 kg
CARGO CAPACITY: 2000 kg
MAX. TOWED WEIGHT: 2000 kg
GROUND CLEARANCE (AXLES): 0.38 m
                 (HULL): 0.53 m
TURNING RADIUS: 10.00 m
MAX. ROAD SPEED: 92.00 km/h
MAX. CROSS-COUNTRY SPEED: 30.00 km/h
MAX. WATER SPEED: 5.00 km/h
FORDING DEPTH: Amphibious
GRADIENT: 60%
SIDE SLOPE: 30%
VERTICAL OBSTACLE: 0.61 m
TRENCH: 0.5 m
ARMOUR CLASS: 100 all around
ARMAMENT: MECAR 90/28 90 mm Light Gun, Main 
          M240C 7.62 mm Machine Gun, Co-Axial
          M240D 7.62 mm Machine Gun, Anti-Aircraft
MAXIMUM RATE OF TURRET, POWER TRAVERSE: 30ø/ second
MAXIMUM RATE OF TURRET, POWER ELEVATION: 30ø/ second
MAIN & CO-AXIAL, GUN ELEVATION/ DEPRESSION: +28ø/ -8ø
TURRET TRAVERSE: 360ø
AMMUNITION: 8/ 37 90 mm, Main (Ready/ Stored)
            400/ 800 7.62 mm, Co-Axial
            200/ 0 7.62 mm, Anti-Aircraft
            4 Anti-Personal, 4 Smoke/ 12 AP, 12 Smoke
SMOKE LAYING EQUIPMENT: 2 x 4 Tube M257 Smoke Launcher
EQUIPMENT: See Attached Sheets
NOTES: 
- The vehicle has a 500 000 candlepower spotlight mounted co-
  axially with the main gun, that will illuminate up to 1.5 kms
  away.  
- The turret is a 2 man turret with Anti-Aircraft MMG mounted to
  the Commanders/ Gunner hatch area.
- Turret traverse can be by Commander or Gunner.
- Winch (Max 9072 kg Tow Limit, 45 m x 12.7 mm Tow Cable).  
- Vehicle is NBCW Proof and Amphibious.
- Tires are 14.50" x 21" Tubeless Tires, with Hutchinson Run Flat
  Insert, which are good for 50 Kms once flat.
- Fusion Engine can be removed and replaced in 1 hour, with
  proper tools and crane.

AMMUNITION:

 MECAR 90 mm Light Gun

  M600 High Explosive Anti-Tank

   * - * - * - * - * - * - * - * - * - * - * - * - * - * ---

  M601 High Explosive

   * - * - * - * - * - * - * - * - * - * - * - * - * - * -
   * - * - * ---

  M602 Smoke

   * - * - * - * - * - * ---

  M621 Canister
 
   * - * - * - * - * - * - * - * ---

 M240C 7.62 mm Co-Axial Machine Gun

  ****************************************************************** - 
  ****************************************************************** - 
  ****************************************************************** --- 

     AP, AP, AP, AP, API-T, API-T

 Short Burst = 6 rds, Medium = 12 rds, Long = 18 rds

 M240D 7.62 mm Anti-Aircraft Machine Gun

  ********************************* --- 

     AP, AP, AP, AP, API-T, API-T

 Short Burst = 6 rds, Medium = 12 rds, Long = 18 rds

 M257 66 mm Smoke/ Anti-Personnel Grenade Launchers

  Left       Right

  SA/AS -    SA/AS -
  SA/AS -    SA/AS -
  SA/AS -    SA/AS -
  SA/AS -    SA/AS ---

  A = Anti-Personal   S = Smoke

 Fired in volleys of 4 or 8 at a time.
 When firing mark off one side of the slash.

 Armbrust 300

 * - * - * - * ---