M800 Armoured Reconnaissance Scout Vehicle

CREW: 3 (Driver, Commander & Gunner)
CONFIGURATION: Tracked
LENGTH: 4.67 m
WIDTH: 2.43
HEIGHT (TURRET): 2.39 m
       (HULL): 
WEIGHT (EMPTY): 8249 kg
       (LOADED): 8890 kg
CARGO CAPACITY: 650 kg 
MAX. TOWED WEIGHT: 2000 kg
GROUND CLEARANCE: 0.41 m
TURNING RADIUS: 4.67 m
MAX. ROAD SPEED: 85.00 km/h
MAX. CROSS-COUNTRY SPEED: 25.00 km/h
MAX. WATER SPEED: 7.00 km/h
FORDING DEPTH: Amphibious
GRADIENT: 60%
SIDE SLOPE: 40%
VERTICAL OBSTACLE: 0.76 m
TRENCH: 1.8 m
ARMOUR CLASS: 100 all around
ARMAMENT: M242 25 mm Automatic Cannon, Gyro-Stabilized, Main 
          M240D 7.62 mm LMG, Pintle, Anti-Aircraft
MAXIMUM RATE OF TURRET, POWER TRAVERSE: 90ø/ second
MAXIMUM RATE OF TURRET, POWER ELEVATION: 90ø/ second
MAIN & CO-AXIAL, GUN ELEVATION/ DEPRESSION: +65ø/ -20ø
AMMUNITION: 444 25 mm, Main (Ready)
            200/ 1200 7.62 mm, Anti-Aircraft (Ready/ Stored
            4 Anti-Personal, 4 Smoke/ 12 AP, 12 Smoke
SMOKE LAYING EQUIPMENT: 2 x 4 Tube M257 Smoke Launcher
EQUIPMENT: See Attached Sheet
NOTES: 
- The turret is a 2 man turret with Anti-Aircraft LMG mounted to
  the Commanders hatch area.
- Turret traverse can be by Commander or Gunner.
- Vehicle is NBCW Proof and Amphibious.
- Fusion Engine can be removed and replaced in 1 hour, with
  proper tools and crane.  Engine slides out the back, on rollers
  and cradle.
- There 64 shoes per track. Each shoe lasts approximately, 1000
  km, with the entire tracks life expected to be 4850 km.
- 4 Road wheels per side. Each wheel is 61 cm x 6 cm.
- Turret basket has an enlarged to accommodate the vehicle
  stores.

AMMUNITION:

 M242 25 mm Chain Gun

  *******************************************************  
  ******************************************************** --- 

     APDS-T, APDS-T, APDS-T, HEI-T

 Short Burst = 4 rds, Medium = 8 rds, Long = 12 rds.

 M240D 7.62 mm LMG

  ********************************* - 
  ********************************* - 
  ********************************* - 
  ********************************* -
  ********************************* - 
  ********************************* - 
  ********************************* --- 

     AP, AP, AP, AP, API-T, API-T

 Short Burst = 6 rds, Medium = 12 rds, Long = 18 rds

 M257 66 mm Smoke/ Anti-Personnel Grenade Launchers

  Left       Right

  SA/AS -    SA/AS -
  SA/AS -    SA/AS -
  SA/AS -    SA/AS -
  SA/AS -    SA/AS ---

  A = Anti-Personal   S = Smoke

 Fired in volleys of 4 or 8 at a time.
 When firing mark off one side of the slash.

 Armbrust 300

  * - * - * - * ---