COMMANDO LAV-600 F Reconnaissance Vehicle

CREW: 4 (Driver, Commander, Loader & Gunner)
CONFIGURATION: 6 x 6
LENGTH: 6.30 m
WIDTH: 2.68 m
HEIGHT (TURRET): 2.74 m
       (HULL): 1.80 m
WEIGHT (EMPTY): 15 000 kg
       (LOADED): 17 010 kg
CARGO CAPACITY: 2000 kg
MAX. TOWED WEIGHT: 2000 kg
GROUND CLEARANCE (AXLES): 0.35 m
                 (HULL): 0.50 m
TURNING RADIUS: 13.25 m
MAX. ROAD SPEED: 84.00 km/h
MAX. CROSS-COUNTRY SPEED: 30.00 km/h
MAX. WATER SPEED: 0 km/h
FORDING DEPTH: 1.07 m
GRADIENT: 60%
SIDE SLOPE: 30%
VERTICAL OBSTACLE: 0.61 m
TRENCH: 0.5 m
ARMOUR CLASS: 100 all around
ARMAMENT: L7A3/ M68 105 mm Low Recoil Gun, Main 
          M240C 7.62 mm Machine Gun, Co-Axial
          M2HB .50 cal Heavy Machine Gun, Anti-Aircraft
MAXIMUM RATE OF TURRET, POWER TRAVERSE: 40ø/ second
MAXIMUM RATE OF TURRET, POWER ELEVATION: 40ø/ second
MAIN & CO-AXIAL, GUN ELEVATION/ DEPRESSION: +20ø/ -7.5ø
TURRET TRAVERSE: 360ø
AMMUNITION: 8/ 28 76 mm, Main (Ready/ Stored)
            400/ 1200 7.62 mm, Co-Axial
            105/ 420 .50 cal, Anti-Aircraft
            4 Anti-Personal, 4 Smoke/ 12 AP, 12 Smoke
SMOKE LAYING EQUIPMENT: 2 x 4 Tube M257 Smoke Launcher
EQUIPMENT: See Attached Sheets
NOTES: 
- The vehicle has a 500 000 candlepower spotlight mounted co-
  axially with the main gun, that will illuminate up to 1.5 kms
  away.  
- The turret is a 2 man turret with Anti-Aircraft MMG mounted to
  the Commander hatch area.
- Turret traverse can be by Commander or Gunner.
- Winch (Max 11 072 kg Tow Limit, 45 m x 12.7 mm Tow Cable).  
- Vehicle is NBCW Proof and Amphibious.
- Tires are 14.50" x 21" Tubeless Tires, with Hutchinson Run Flat Insert
  which are good for 50 Kms once flat.
- Fusion Engine can be removed and replaced in 1 hour, with
  proper tools and crane.

AMMUNITION:

 L7A3/ M68 105 mm Low Recoil Gun

  M393 High Explosive Plastic with Tracer

   * - * - * - * - * - * - * - * - * - * - * ---

  M456 High Explosive Anti-Tank with Tracer

   * - * - * - * - * - * - * - * - * - * ---

  M392A2 Armour Piercing Discarding Sabot with Tracer

   * - * - * - * - * - * - * - * --- 

  M494A3 Anti-Personnel (Flechette) with Tracer
 
   * - * - * - * - * - * - * ---

 M240C 7.62 mm Co-Axial Machine Gun

  ****************************************************************** - 
  ****************************************************************** - 
  ****************************************************************** - 
  ****************************************************************** --- 

     AP, AP, AP, AP, API-T, API-T

 Short Burst = 6 rds, Medium = 12 rds, Long = 18 rds

 M2HB HMG .50 cal

  ************ -
  ************ -
  ************ -
  ************ -
  ************ ---

 Short Burst = 10 rds, Medium = 20 rds, Long = 30 rds.

 M257 66 mm Smoke/ Anti-Personnel Grenade Launchers

  Left      Right

  SA/AS -    SA/AS -
  SA/AS -    SA/AS -
  SA/AS -    SA/AS -
  SA/AS -    SA/AS ---

  A = Anti-Personal   S = Smoke

 Fired in volleys of 4 or 8 at a time.
 When firing mark off one side of the slash.

 Armbrust 300

 * - * - * - * ---