COMMANDO LAV-300 F AMBULANCE

CREW: 3 (Driver, 2 Medics) + 8 Ambulatory or 4 Litter Patients or
      combination of litter and ambulatory patients
CONFIGURATION: 6 x 6
LENGTH: 6.40 m
WIDTH: 2.54 m
HEIGHT: 2.65 m
WEIGHT (EMPTY): 10 918 kg
       (LOADED): 12 418 kg
CARGO CAPACITY: 2000 kg
MAX. TOWED WEIGHT: 2000 kg
GROUND CLEARANCE (AXLES): 0.38 m
                 (HULL): 0.53 m
TURNING RADIUS: 10.00 m
MAX. ROAD SPEED: 92.00 km/h
MAX. CROSS-COUNTRY SPEED: 30.00 km/h
MAX. WATER SPEED: 5.00 km/h
FORDING DEPTH: Amphibious
GRADIENT: 60%
SIDE SLOPE: 30%
VERTICAL OBSTACLE: 0.61 m
TRENCH: 0.5 m
ARMOUR CLASS: 100 all around
ARMAMENT: None
AMMUNITION: 4 Anti-Personal, 4 Smoke/ 12 AP, 12 Smoke
SMOKE LAYING EQUIPMENT: 2 x 4 Tube M257 Smoke Launcher
EQUIPMENT: See Attached Sheets
NOTES: 
- Vehicle is the same as the Command and Control vehicle from the
  outside with the exception of, a rear ramp installed.
- Stretchers and walking wounded are loaded through rear ramp.
- The roof area has no provision for a roof mounted hatch or
  weapons station. 
- Full vehicle air conditioning is provided for patient comfort.
- Winch (Max 9072 kg Tow Limit, 45 m x 12.7 mm Tow Cable).  
- Vehicle is NBCW Proof and Amphibious.
- Tires are 14.50" x 21" Tubeless Tires, with Hutchinson Run Flat
  Insert, which are good for 50 Kms once flat.
- Fusion Engine can be removed and replaced in 1 hour, with
  proper tools and crane.

AMMUNITION:

 M257 66 mm Smoke/ Anti-Personnel Grenade Launchers

  Left       Right

  SA/AS -    SA/AS -
  SA/AS -    SA/AS -
  SA/AS -    SA/AS -
  SA/AS -    SA/AS ---

  A = Anti-Personal  S = Smoke

 Fired in volleys of 4 or 8 at a time.
 When firing mark off one side of the slash.

 Armbrust 300

 * - * - * - * ---