COMMANDO V-150 SF

CREW: 3 (Driver, Commander & Gunner) + 1 Passenger
CONFIGURATION: 4 x 4
LENGTH: 6.14 m
WIDTH: 2.26 m
HEIGHT (TURRET): 2.53 m
       (HULL): 1.98 m
WEIGHT (EMPTY): 8981 kg
       (LOADED): 10 106 kg
CARGO CAPACITY: 2000 kg
MAX. TOWED WEIGHT: 2000 kg
GROUND CLEARANCE (AXLES): 0.38 m
                 (HULL): 0.65 m
TURNING RADIUS: 8.50 m
MAX. ROAD SPEED: 88.50 km/h
MAX. CROSS-COUNTRY SPEED: 30.00 km/h
MAX. WATER SPEED: 5.00 km/h
FORDING DEPTH: Amphibious
GRADIENT: 60%
SIDE SLOPE: 30%
VERTICAL OBSTACLE: 0.91 m
TRENCH: 0.5 m
ARMOUR CLASS: 100 all around
ARMAMENT: M2HB .50 cal HMG, Main & Co-Axial
MAXIMUM RATE OF TURRET, POWER TRAVERSE (FAST): 45ø/ second
MAXIMUM RATE OF TURRET, MANUAL ELEVATION: 6ø/ second
MAIN & CO-AXIAL, GUN ELEVATION/ DEPRESSION: +55ø/ -10ø Manual
TURRET TRAVERSE: 360ø
AMMUNITION: 420/ 1260 .50 cal (Ready/ Stored)
            4 Anti-Personal, 4 Smoke/ 12 AP, 12 Smoke
SMOKE LAYING EQUIPMENT: 2 x 4 Tube M257 Smoke Launcher
EQUIPMENT: See Attached Sheets
NOTES: 
- The vehicle has a 500 000 candlepower spotlight mounted co-
  axially with the main gun, that will illuminate up to 1.5 kms
  away.  
- The turret is a 1 man turret.
- Winch (Max 4536 kg Tow Limit, 48.76 m x 9.5 mm Tow Cable).  
- Vehicle is NBCW Proof and Amphibious.
- Tires are 14.50" x 21" Tubeless Tires, with Hutchinson Run Flat Insert
  which are good for 50 Kms once flat.
- Fusion Engine can be removed and replaced in 1 hour, with
  proper tools and crane.

AMMUNITION:

 M2HB HMG .50 cal

  Main                           Co-Axial

  ********************* -        ********************* -  
  ********************* -        ********************* -
  ********************* -        ********************* - 
  ********************* ---      ********************* ---

 Short Burst = 10 rds, Medium = 20 rds, Long = 30 rds.

 M257 66 mm Smoke/ Anti-Personnel Grenade Launchers

  Left       Right

  SA/AS -    SA/AS -
  SA/AS -    SA/AS -
  SA/AS -    SA/AS -
  SA/AS -    SA/AS ---

  A = Anti-Personal   S = Smoke

 Fired in volleys of 4 or 8 at a time.
 When firing mark off one side of the slash.

 Armbrust 300

 * - * - * - * ---