COMMANDO LAV-300 F IMPROVED TOW VEHICLE (ITV), UNDER ARMOUR

CREW: 3 (Driver, Commander/ Gunner & Loader)
CONFIGURATION: 6 x 6
LENGTH: 6.40 m
WIDTH: 2.54 m
HEIGHT (TURRET, DEPLOYED): 3.50 m
       (TURRET, STOWED): 3.06 m
       (HULL): 1.98 m
WEIGHT (EMPTY): 13 318 kg
       (LOADED): 15 818 kg
CARGO CAPACITY: 2000 kg
MAX. TOWED WEIGHT: 2000 kg
GROUND CLEARANCE (AXLES): 0.38 m
                 (HULL): 0.53 m
TURNING RADIUS: 10.00 m
MAX. ROAD SPEED: 92.00 km/h
MAX. CROSS-COUNTRY SPEED: 30.00 km/h
MAX. WATER SPEED: 5.00 km/h
FORDING DEPTH: Amphibious
GRADIENT: 60%
SIDE SLOPE: 30%
VERTICAL OBSTACLE: 0.61 m
TRENCH: 0.5 m
ARMOUR CLASS: 100 all around
ARMAMENT: TOW Anti-Tank Guided Weapon x2, Main 
          M240D 7.62 mm Machine Gun, Cupola, Anti-Aircraft
MAXIMUM RATE OF TURRET, POWER TRAVERSE: 35ø/ second
MAXIMUM RATE OF LAUNCHER, POWER ELEVATION: 34ø/ second
MAXIMUM RATE OF LAUNCHER, POWER DEPRESSION: 30ø/ second
LAUNCHER ELEVATION/ DEPRESSION: +34ø/ -30ø
TURRET TRAVERSE: 360ø
AMMUNITION: 2/ 8 TOW (Ready/ Stored), Main
            200/ 600 7.62 mm, Anti-Aircraft
            4 Anti-Personal, 4 Smoke/ 12 AP, 12 Smoke
SMOKE LAYING EQUIPMENT: 2 x 4 Tube M257 Smoke Launcher
EQUIPMENT: See Attached Sheets
NOTES: 
- TOW (Tube-launched, Optically-guided, Wire-tracked)
- Turret is the Emerson Improved TOW Launcher, as installed on
  the M901 ITV. Development began in Late 1975 and became the
  standard under Armour TOW launcher in late 1976.
- The cupola is 1 man turret with Anti-Aircraft MMG mounted to
  the rear of the hatch area.  The armoured TOW launcher assembly
  is attached above this.
- The launcher can fire any of the TOW missile variants, BGM-71A
  Basic TOW, BGM-71B Extended Range TOW (ER-TOW), BGM-71C
  Improved TOW (I-TOW) or BGM-71D TOW 2, BGM-71E TOW 2A or
  BGM-71F TOW 2B.
- Once the ITV has stopped it takes only 20 seconds for the
  launcher to be elevated and the target engaged.
- Time from first-round impact to second-round triggering with a
  12.5ø target separation is 4.25 seconds.
- When travelling, the system is retracted onto the top of the
  hull, to the rear of the cupola hatch.
- To reload launcher(s), the unit is tilted back toward the rear
  of the vehicle.  Where the loader opens the armoured roof
  hatch.  Reaches out and replaces the expended TOW canisters
  with fresh rounds.
- Winch (Max 9072 kg Tow Limit, 45 m x 12.7 mm Tow Cable).  
- Vehicle is NBCW Proof and Amphibious.
- Tires are 14.50" x 21" Tubeless Tires, with Hutchinson Run Flat
  Insert, which are good for 50 Kms once flat.
- Fusion Engine can be removed and replaced in 1 hour, with
  proper tools and crane.

AMMUNITION:

 BGM-71A Basic TOW or Any Of The Variants

  * * - * * - * * - * * - * * --- 

 M240D 7.62 mm Anti-Aircraft Machine Gun

  ********************************* - 
  ********************************* - 
  ********************************* - 
  ********************************* --- 

     AP, AP, AP, AP, API-T, API-T

 Short Burst = 6 rds, Medium = 12 rds, Long = 18 rds

 M257 66 mm Smoke/ Anti-Personnel Grenade Launchers

  Left       Right

  SA/AS -    SA/AS -
  SA/AS -    SA/AS -
  SA/AS -    SA/AS -
  SA/AS -    SA/AS ---

  A = Anti-Personal  S = Smoke

 Fired in volleys of 4 or 8 at a time.
 When firing mark off one side of the slash.

Armbrust 300

 * - * - * - * ---