M825 1/4-ton Weapons Carrier w/ M40A2 106 mm Recoilless Rifle

CREW: 1 (Driver) + 3 (Gunner, Loader & Squad Leader) 
CONFIGURATION: 4 x 4
LENGTH: 3.65 m
WIDTH: 1.94 m
HEIGHT (OVERALL): 1.62 m
       (REDUCED): 1.35m
WEIGHT (EMPTY): 1174 kg
       (LOADED): 1959 kg
MAX LOAD (ROAD): 785 kg
         (CROSS-COUNTRY): 785 kg
MAX. TOWED LOAD (ROAD): Not Authorised
                (CROSS-COUNTRY): Not Authorised
GROUND CLEARANCE (AXLES): 0.21 m
TURNING RADIUS: 5.63 m
MAX. ROAD SPEED: 90 km/h
MAX. CROSS-COUNTRY SPEED: 30 km/h
FORDING DEPTH (without PREPARATION): 0.53 m
              (with PREPARATION): 1.52 m
GRADIENT: 50%
SIDE SLOPE: 30%
VERTICAL OBSTACLE: n/a
ARMOUR CLASS: F: 12, R: 9, S: 9, T: 0, B: 5
ARMAMENT: M40A2 106 mm Recoilless Rifle
AMMUNITION: 0 / 6  (Ready/ Stored)
SMOKE LAYING EQUIPMENT: None Normally Installed
EQUIPMENT: See Attached Sheets
NOTES: 
- With the M40A2 recoilless rifle mounted, the rifle can be
  traversed 112o to the left from centre, and 115o to the right
  from centre. 25o to each side of centre is an area of no fire,
  to prevent any damage to the M825 weapons carrier.
- The ammunition is stored on the floor, in the rear of the M825.
- 1 fold down seat is provided to either side (facing the rifle)
  of the recoilless rifle  
- Tires are 7.00" x 16".
- The Autonav system is installed below the front passenger seat
  in the old battery compartment, with a read out screen mounted
  on lower portion of the centre of the dash board.
- All vehicles start out painted olive drab, and can and should
  be adapted to match local environmental conditions.
- Fusion Engine can be removed and replaced in « an hour, with
  proper tools and crane.
- Payload includes crew, personal gear, BII (Basic Issue Items),
  special kits & equipment and trailer tongue weight.

AMMUNITION:

 106 mm M40A2 Recoilless Rifle

 M344A1 HEAT

  * - * - * - - -
 
 M346A1 HEP-T

  * - *  - - -

 M581 APERS-T

  *  - - -


 Armbrust 300

  * - *  - - -

