ASSAULT RIFLES (United States of America)
                    
XM177E1 (M609) & XM177E2 (M629) "COLT COMMANDO"

Nation: US 
Weapon Type: Assault Rifle
Caliber: 5.56 x 45 mm (.223 Remington)
Muzzle Velocity: 2750 fps
Length (E1; Extended): 78.70 cm
       (E1; Collapsed): 71.90 cm
       (E2; Extended): 82.60 cm
       (E2; Collapsed): 75.70 cm
Weight(E1): 2.36 kg
      (E2): 2.43 kg
Type of Fire: Selective; Semiautomatic or Full automatic 
Rate of Fire (Single Shot): 45 to 65 rpm
             (Automatic): 150 to 200 rpm
             (Cyclic): 700 to 800 rpm
Feed Device: 20 or 30 round magazine
Magazine Weight: 20: 0.32 kg, 30: 0.46 kg
Load Time: 3 seconds
RANGE
 Point Blank   C(9+)   M(12+)   L(14+)   Ex(18+)
     2 m.      50 m.   130 m.   250 m.   350 m.
Damage DM:
     +2        +2      +1       -        -
Penetration: 12
Recoil: +1 
Failure: 12+ (10+ in bad conditions without maintenance)

M16A1 (M603)

Nation: US 
Weapon Type: Assault Rifle
Caliber: 5.56 x 45 mm (.223 Remington)
Muzzle Velocity: 3250 fps
Length: 99 cm
Weight: 2.95 kg
Type of Fire: Selective; Semiautomatic or Full automatic 
Rate of Fire (Single Shot): 45 to 65 rpm
             (Automatic): 150 to 200 rpm
             (Cyclic): 700 to 800 rpm
Feed Device: 20 or 30 round magazine
Magazine Weight: 20: 0.32 kg, 30: 0.46 kg
Load Time: 3 seconds
RANGE
 Point Blank   C(9+)   M(12+)   L(14+)   Ex(18+)
     2 m.      50 m.   150 m.   300 m.   450 m.
Damage DM:
     +2        +2      +1       -        -
Penetration: 15
Recoil: -1 
Failure: 12+ (10+ in bad conditions without maintenance)

M16A2 (M645)

Nation: US 
Weapon Type: Assault Rifle
Caliber: 5.56 x 45 mm (.223 Remington)
Muzzle Velocity: 3100 fps
Length: 100 cm
Weight: 3.58 kg
Type of Fire: Selective; Semiautomatic or 3 rd Burst 
Rate of Fire (Single Shot): 45 to 65 rpm
             (Automatic): 150 rpm
             (Cyclic): 600 to 900 rpm
Feed Device: 20 or 30 round magazine
Magazine Weight: 20: 0.32 kg, 30: 0.46 kg
Load Time: 3 seconds
RANGE
 Point Blank   C(9+)   M(12+)   L(14+)   Ex(18+)
     2 m.      50 m.   150 m.   300 m.   450 m.
Damage DM:
     +2        +2      +1       -        -
Penetration: 15
Recoil: -1 
Failure: 12+ (10+ in bad conditions without maintenance)

M16A3 (M701)

Nation: US 
Weapon Type: Assault Rifle
Caliber: 5.56 x 45 mm (.223 Remington)
Muzzle Velocity: 3100 fps
Length: 100 cm
Weight: 3.58 kg
Type of Fire: Selective; Semiautomatic or Full automatic 
Rate of Fire (Single Shot): 45 to 65 rpm
             (Automatic): 150 rpm
             (Cyclic): 600 to 900 rpm
Feed Device: 20 or 30 round magazine
Magazine Weight: 20: 0.32 kg, 30: 0.46 kg
Load Time: 3 seconds
RANGE
 Point Blank   C(9+)   M(12+)   L(14+)   Ex(18+)
     2 m.      50 m.   150 m.   300 m.   450 m.
Damage DM:
     +2        +2      +1       -        -
Penetration: 15
Recoil: -1 
Failure: 12+ (10+ in bad conditions without maintenance)

M16A4 (M901)

Nation: US 
Weapon Type: Assault Rifle
Caliber: 5.56 x 45 mm (.223 Remington)
Muzzle Velocity: 3250 fps
Length: 100 cm
Weight (Carrying Handle Removed): 3.42 kg
       (Carrying Handle Mounted): 3.82 kg
Type of Fire: Selective; Semiautomatic or Full automatic 
Rate of Fire (Single Shot): 45 to 65 rpm
             (Automatic): 150 to 200 rpm
             (Cyclic): 600 to 900 rpm
Feed Device: 20 or 30 round magazine
Magazine Weight: 20: 0.32 kg, 30: 0.46 kg
Load Time: 3 seconds
RANGE
 Point Blank   C(9+)   M(12+)   L(14+)   Ex(18+)
     2 m.      100 m.  250 m.   375 m.   525 m.
Damage DM:
     +2        +2      +1       -        -
Penetration: 15
Recoil: -1 
Failure: 12+ (10+ in bad conditions without maintenance)
NOTE: This is a updated version of the A2/A3.  Main difference is
the integrated carrying handle/ sight is removable and a
Picatinny Rail Mounting system has been added.  For backup
situations, a slip on iron rear sight can be added to the rail
system.

M16A1 CARBINE (M653)

Nation: US 
Weapon Type: Assault Rifle
Caliber: 5.56 x 45 mm (.223 Remington)
Muzzle Velocity: 3020 fps
Length (Extended): 83.80 cm
       (Collapsed): 75.70 cm
Weight: 2.54 kg
Type of Fire: Selective; Semiautomatic or Full automatic 
Rate of Fire (Single Shot): 45 to 65 rpm
             (Automatic): 150 to 200 rpm
             (Cyclic): 700 to 800 rpm
Feed Device: 20 or 30 round magazine
Magazine Weight: 20: 0.32 kg, 30: 0.46 kg
Load Time: 3 seconds
RANGE
 Point Blank   C(9+)   M(12+)   L(14+)   Ex(18+)
     2 m.      50 m.   140 m.   275 m.   325 m.
Damage DM:
     +2        +2      +1       -        -
Penetration: 13
Recoil: -1 
Failure: 12+ (10+ in bad conditions without maintenance)
NOTE: M16A1 Carbine CAN NOT accept the M203/ M203A1 grenade
launcher.

M16A2 CARBINE (M723)

Nation: US 
Weapon Type: Assault Rifle
Caliber: 5.56 x 45 mm (.223 Remington)
Muzzle Velocity: 3020 fps
Length (Extended): 83.80 cm
       (Collapsed): 75.70 cm
Weight: 2.54 kg
Type of Fire: Selective; Semiautomatic or Full automatic 
Rate of Fire (Single Shot): 45 to 65 rpm
             (Automatic): 150 to 200 rpm
             (Cyclic): 700 to 800 rpm
Feed Device: 20 or 30 round magazine
Magazine Weight: 20: 0.32 kg, 30: 0.46 kg
Load Time: 3 seconds
RANGE
 Point Blank   C(9+)   M(12+)   L(14+)   Ex(18+)
     2 m.      50 m.   140 m.   275 m.   325 m.
Damage DM:
     +2        +2      +1       -        -
Penetration: 13
Recoil: -1 
Failure: 12+ (10+ in bad conditions without maintenance)
NOTE: The M16A2 Carbine CAN NOT accept the M203/ M203A1 grenade
launcher.

M4 CARBINE (M720) & (M727)

Nation: US 
Weapon Type: Assault Rifle
Caliber: 5.56 x 45 mm (.223 Remington)
Muzzle Velocity: 2900 fps
Length (Extended): 83.80 cm
       (Collapsed): 75.70 cm
Weight: 3.32 kg
Type of Fire: (M720) Selective; Semiautomatic or 3 rd Burst 
              (M727) Selective; Semiautomatic or Full automatic
Rate of Fire (Single Shot): 45 to 65 rpm
             (Automatic): 150 to 200 rpm
             (Cyclic): 700 to 800 rpm
Feed Device: 20 or 30 round magazine
Magazine Weight: 20: 0.32 kg, 30: 0.46 kg
Load Time: 3 seconds
RANGE
 Point Blank   C(9+)   M(12+)   L(14+)   Ex(18+)
     2 m.      50 m.   140 m.   275 m.   325 m.
Damage DM:
     +2        +2      +1       -        -
Penetration: 12
Recoil: -1 
Failure: 12+ (10+ in bad conditions without maintenance)

M4A1 CARBINE (M927)

Nation: US 
Weapon Type: Assault Rifle
Caliber: 5.56 x 45 mm (.223 Remington)
Muzzle Velocity: 2760 fps
Length (Extended): 84.77 cm
       (Collapsed): 76.54 cm
Weight (Carrying Handle Installed): 2.89 kg 
       (Carrying Handle Removed): 
Type of Fire: Selective; Semiautomatic or Full automatic 
Rate of Fire (Single Shot): 45 to 65 rpm
             (Automatic): 150 to 200 rpm
             (Cyclic): 600 to 900 rpm
Feed Device: 20 or 30 round magazine
Magazine Weight: 20: 0.32 kg, 30: 0.46 kg
Load Time: 3 seconds
RANGE
 Point Blank   C(9+)   M(12+)   L(14+)   Ex(18+)
     2 m.      50 m.   140 m.   275 m.   325 m.
Damage DM:
     +2        +2      +1       -        -
Penetration: 12
Recoil: -1 
Failure: 12+ (10+ in bad conditions without maintenance)
NOTE: This is a updated version of the M4 Carbine.  The
integrated carrying handle/ sight is removable and a Picatinny
Rail Mounting system has been added.  For backup situations, flip
up iron sights have been integrated.

COMMANDO ASSAULT RIFLE (M733 & M735) 

Nationality: US 
Weapon Type: Assault Rifle
Caliber: 5.56 x 45 mm (.223 Remington)
Muzzle Velocity: 2610 fps
Length (Extended): 76.00 cm
       (Collapsed): 68.00 cm
Weight: 2.44 kg
Type of Fire (M733): Selective; Single shot or Full automatic
             (M735): Selective; Single shot or 3 Rd Burst  
Rate of Fire (Single Shot): 45 to 65 rpm
             (Automatic): 150 to 200 rpm
             (Cyclic): 600 to 900 rpm
Feed Device: 20 or 30 round magazine
Magazine Weight: 20: 0.32 kg, 30: 0.46 kg
Load Time: 3 seconds
RANGE
 Point Blank   C(9+)   M(12+)   L(14+)   Ex(18+)
     2 m.      50 m.   140 m.   275 m.   400 m.
Damage DM:
     +2        +2      +1       -        -
Penetration: 11
Recoil: -1 
Failure: 12+ (10+ in bad conditions without maintenance)
Note: The M733/ M735 Commando is the smallest and most compact
version of the M16A2 rifle.  Developed to provide a robust weapon
with compact dimensions allowing speed of action.  The Commando
can be carried in the slung position with a minimum of
inconvenience and bulk, much like a sub-machine gun.  It can
provide instant, accurate and effective fire under all combat
conditions.  The M735s mechanical components are interchangeable
with those of the M16A2 rifle, the M733 mechanical components are
interchangeable with the M16A3 rifle.  It accepts all M16
magazines.  The Commando CAN NOT accept the M203 or M203A1
grenade launcher.

COMMANDO ASSAULT RIFLE (M933 & M935) 

Nationality: US 
Weapon Type: Assault Rifle
Caliber: 5.56 x 45 mm (.223 Remington)
Muzzle Velocity: 2610 fps
Length (Extended): 76.00 cm
       (Collapsed): 68.00 cm
Weight (Carrying Handle Mounted): 2.12 kg
       (Carrying Handle Removed):  kg
Type of Fire (M933): Selective; Single shot or Full automatic
             (M935): Selective; Single shot or 3 Rd Burst  
Rate of Fire (Single Shot): 45 to 65 rpm
             (Automatic): 150 to 200 rpm
             (Cyclic): 600 to 900 rpm
Feed Device: 20 or 30 round magazine
Magazine Weight: 20: 0.32 kg, 30: 0.46 kg
Load Time: 3 seconds
RANGE
 Point Blank   C(9+)   M(12+)   L(14+)   Ex(18+)
     2 m.      50 m.   140 m.   275 m.   400 m.
Damage DM:
     +2        +2      +1       -        -
Penetration: 11
Recoil: -1 
Failure: 12+ (10+ in bad conditions without maintenance)
Note: The M933/ M935 Commando is the same as the M733/ M735
models, with the difference being the carrying handle/ rear sight
can be removed to provide access to the Picatinny Rail Mounting
System.  The Commando CAN NOT accept the M203 or M203A1 grenade
launcher.

M16K ASSAULT CARBINE

Nationality: US 
Weapon Type: Assault Rifle
Caliber: 5.56 x 45 mm (.223 Remington)
Muzzle Velocity: 2400 fps
Length (Extended): 68.60 cm
       (Collapsed): 61.00 cm
Weight: 2.50 kg
Type of Fire: Selective; Single shot or Full automatic
Rate of Fire (Single Shot): 45 to 65 rpm
             (Automatic): 150 to 200 rpm
             (Cyclic): 550 to 600 rpm
Feed Device: 20 or 30 round magazine
Magazine Weight: 20: 0.32 kg, 30: 0.46 kg
Load Time: 3 seconds
RANGE
 Point Blank   C(9+)   M(12+)   L(14+)   Ex(18+)
     2 m.      50 m.   140 m.   275 m.   400 m.
Damage DM:
     +2        +2      +1       -        -
Penetration: 11
Recoil: - 
Failure: 12+ (10+ in bad conditions without maintenance)
Note: The M16K Assault Carbine is the smallest and one of the
lightest of the M16 variants. Developed to provide a robust
weapon that can be carried in the confined spaces of aircraft or
vehicles. The flash suppressor eliminates all traces of muzzle
flash. It accepts all M16 magazines. The M16K CAN NOT accept the
M203 or M203A1 grenade launcher.

M16X ASSAULT CARBINE

Nationality: US 
Weapon Type: Assault Rifle
Caliber: 5.56 x 45 mm (.223 Remington)
Muzzle Velocity: 1558 fps
Length (Extended): 59.20 cm
       (Collapsed): 51.00 cm
Weight: 2.38 kg
Type of Fire: Selective; Single shot or Full automatic
Rate of Fire (Single Shot): 45 to 65 rpm
             (Automatic): 150 to 200 rpm
             (Cyclic): 650 to 700 rpm
Feed Device: 20 or 30 round magazine
Magazine Weight: 20: 0.32 kg, 30: 0.46 kg
Load Time: 3 seconds
RANGE
 Point Blank   C(9+)   M(12+)   L(14+)   Ex(18+)
     2 m.      40 m.   125 m.   200 m.   275 m.
Damage DM:
     +2        +2      +1       -        -
Penetration: 7
Recoil: -
Failure: 12+ (10+ in bad conditions without maintenance)
Note: The M16X Assault Carbine is one of the smallest of the M16
variants. Developed to provide a robust weapon that can be
carried concealed under a coat or jacket. The flash suppressor
eliminates all traces of muzzle flash. It accepts all M16
magazines. The M16X CAN NOT accept the M203 or M203A1 grenade
launcher.

M2 Carbine

Nation: US 
Weapon Type: Carbine
Caliber: .30 Carbine
Muzzle Velocity: 1968 fps
Length: 90.50 cm
Weight: 2.36 kg
Type of Fire: Selective; Semiautomatic or Full automatic  
Rate of Fire: 750 rpm
Feed Device: 15 or 30 round magazine
Magazine Weight: 15: 0.26 kg, 30: 0.53 kg
Load Time: 3 seconds
RANGE
 Point Blank   C(9+)   M(12+)   L(14+)   Ex(18+)
     2 m.      50 m.   120 m.   215 m.    300 m.
Damage DM:
     +2        +1      -        -         -
Penetration: 12
Recoil: - 
Failure: 12+

RUGER AC-556F SELECTIVE FIRE WEAPON

Nation: US 
Weapon Type: Assault Rifle
Caliber: 5.56 x 45 mm (.223 Remington)
Muzzle Velocity: 3297 fps
Length: 94.60 cm
Weight: 2.89 kg
Type of Fire: Selective: 3 rd Burst or Full automatic  
Feed Device: 20 or 30 round magazine
Magazine Weight: 20: 0.41 kg, 30: 0.58 kg
Load Time: 3 seconds
RANGE
 Point Blank   C(9+)   M(12+)   L(14+)   Ex(18+)
     2 m.      50 m.   120 m.   215 m.    300 m.
Damage DM:
     +2        +2      +1       -         -
Penetration: 14
Recoil: - 
Failure: 12+

RUGER AC-556K SELECTIVE FIRE WEAPON

Nation: US 
Weapon Type: Assault Rifle
Caliber: 5.56 x 45 mm (.223 Remington)
Muzzle Velocity: 2715 fps
Length (Folded): 58.40 cm
       (Extended): 82.60 cm
Weight: 3.14 kg
Type of Fire: Selective; Semiautomatic, 3 rd Burst or Full
                         automatic  
Rate of Fire: 750 rpm
Feed Device: 20 or 30 round magazine
Magazine Weight: 20: 0.41 kg, 30: 0.58 kg
Load Time: 3 seconds
RANGE
 Point Blank   C(9+)   M(12+)   L(14+)   Ex(18+)
W/ Stock
     2 m.      50 m.   120 m.   215 m.    300 m.
W/O Stock
     2 m.      50 m.   100 m.   190 m.    225 m.
Damage DM:
     +2        +2      +1       -         -
Penetration: 14
Recoil: - 
Failure: 12+

RUGER MINI-14

Nation: US 
Weapon Type: Assault Rifle
Caliber: 5.56 x 45 mm (.223 Remington)
Muzzle Velocity: 3297 fps
Length: 95 cm
Weight: 2.90 kg
Type of Fire; Semiautomatic  
Feed Device: 20 or 30 round magazine
Magazine Weight: 20: 0.41 kg, 30: 0.58 kg
Load Time: 3 seconds
RANGE
 Point Blank   C(9+)   M(12+)   L(14+)   Ex(18+)
     2 m.      50 m.   120 m.   215 m.    300 m.
Damage DM:
     +2        +2      +1       -         -
Penetration: 14
Recoil: - 
Failure: 12+

M1/ M1A1 Carbine

Nation: US 
Weapon Type: Carbine
Caliber: .30 Carbine
Muzzle Velocity: 1968 fps
Length (M1): 90.50 cm
       (M1A1): Extended; 90 cm
       (M1A1): Folded; 64.80 cm
Weight (M1): 2.36 kg
       (M1A1): 2.53 kg
Type of Fire; Semiautomatic  
Feed Device: 15 or 30 round magazine
Magazine Weight: 15: 0.26 kg, 30: 0.53 kg
Load Time: 3 seconds
RANGE
 Point Blank   C(9+)   M(12+)   L(14+)   Ex(18+)
     2 m.      50 m.   120 m.   215 m.    300 m.
Damage DM:
     +2        +1      -        -         -
Penetration: 12
Recoil: - 
Failure: -

Armalite AR-18 

Nation: US 
Weapon Type: Assault Rifle
Caliber: 5.56 x 45 mm (.223 Remington)
Muzzle Velocity: 3280 fps
Length (Extended): 94 cm
       (Folded): 74 cm
Weight: 3.17 kg
Type of Fire: Selective; Semiautomatic or Full automatic 
Rate of Fire (Single Shot): 40 rpm
             (Automatic): 80 rpm
             (Cyclic): 800 rpm
Feed Device: 20, 30  or 40 round magazine
Magazine Weight: 20: 0.33 kg, 30: 0.48 kg, 40: 0.91 kg
Load Time: 3 seconds
RANGE
 Point Blank   C(9+)   M(12+)   L(14+)   Ex(18+)
     2 m.      50 m.   150 m.   300 m.    450 m.
Damage DM:
     +2        +2      +1       -         -
Penetration: 14
Recoil: -1 
Failure: 12+ (10+ in bad conditions without maintenance)
NOTE: The Butt stock folds to the side of the weapon.