VULCAN-COMMANDO V-150 SF SPADS (Self-Propelled Air Defence
System) 

CREW: 4 (Driver, Commander, Gunner & Radio Operator)
CONFIGURATION: 4 x 4
LENGTH: 6.40 m
WIDTH: 2.26 m
HEIGHT (TURRET): 2.89 m
       (HULL): 1.98 m
WEIGHT (EMPTY): 9006 kg
       (LOADED): 10 206 kg
CARGO CAPACITY: 2000 kg
MAX. TOWED WEIGHT: 2000 kg
GROUND CLEARANCE (AXLES): 0.38 m
                 (HULL): 0.65 m
TURNING RADIUS: 8.50 m
MAX. ROAD SPEED: 88.50 km/h
MAX. CROSS-COUNTRY SPEED: 30.00 km/h
MAX. WATER SPEED: 5.00 km/h
ACCELERATION (0 - 32.2 km/h): 10 seconds
FORDING DEPTH: Amphibious
GRADIENT: 60%
SIDE SLOPE: 30%
VERTICAL OBSTACLE: 0.91 m
TRENCH: 0.5 m
ARMOUR CLASS: 100 all around
ARMAMENT: M61A1 20 mm Vulcan Air Defence System, Main 
MAXIMUM RATE OF TURRET, POWER TRAVERSE: 60ø/ second
MAXIMUM RATE OF TURRET, POWER ELEVATION: 45ø/ second
GUN ELEVATION/ DEPRESSION: +80ø/ -5ø
TURRET TRAVERSE: 360ø
AMMUNITION: 1300/ 0 20 mm (Ready/ Stored), Main
EQUIPMENT: See Attached Sheets
NOTES: 
- The turret is a 1 man turret.
- Turret traverse can be by Commander or Gunner.
- Winch (Max 4536 kg Tow Limit, 48.76 m x 9.5 mm Tow Cable).
- Vehicle is NBCW Proof and Amphibious.
- Tires are 14.50" x 21" Tubeless Tires, with Hutchinson Run Flat
  Insert, which are good for 40 Kms once flat.
- Fusion Engine can be removed and replaced in 1 hour, with
  proper tools and crane.
- 3 hydraulic stabilization jacks are mounted to the hull, 1
  front and 2 rear side mounted.  Lowered to provide a more
  stable firing platform for air defence operations.  The jacks
  are controlled from inside the vehicle.
- The system has 4 operational modes.
     Radar: which is the most accurate of the three anti-aircraft
     engagement modes.  The radar supplies continuous range and
     range rate information to the system's analogue computer so
     that computations for the gyro lead sight can be made.
     Manual: in which the gunner estimates the engagement range
     and target speed and then manually enters them on the
     control panel.
     External: in which a second person off-mount estimates the
     target's range and enters the data on an hand-held
     potentiometer connected to the fire-control system by a
     cable.
     Ground: in which the gyro sight is not operated and the lead
     angle not computed.  The sight is mechanically caged to zero
     lead and 7 mils of super-elevation.
- Gunner can select either 10, 30, 60 or 100 round bursts 

AMMUNITION:

 M61A1 20 mm Vulcan Air-Defence System

  ***************************************************************
  ***************************************************************
  **** ---

 Short Burst = 10 rds, Medium = 30 rds, Long = 60 rds,
 Ext. Long = 100 rds.

 Armbrust 300

  * - * - * - * ---
