RECOILLESS RIFLES

M20 75 mm RECOILLESS RIFLE

Nationality: U.S.
Weapon Type: Man Portable Recoilless Rifle
Caliber: 75 mm
Length: 208 cm
Weight: 57 kg (Rifle)
        15 kg (M74 Mount)
Type of Fire: Single shot
Rate of Fire: 1 per combat round
Feed Device: Single round, breach loaded
Ammunition Types: M310A1 HEAT, M309A1 HE, M308A1 WP
Backblast 0 to 25 m: 100 Bp
          25 to 50 m: 50 Bp
Target Area: Range/ 50; Minimum = 5 m
RANGE
 Minimum      C(9+)  M(12+)  L(14+)  Ex(18+)
   20 m.      250 m. 500 m.  1000 m. 6000 m.
Failure: 11+

M67 90 mm RECOILLESS RIFLE

Nationality: U.S.
Weapon Type: Man Portable Recoilless Rifle
Caliber: 90 mm
Length: 135 cm
Weight: 15.88 kg
Type of Fire: Single shot
Rate of Fire: 1 per combat round
Feed Device: Single round, breach loaded
Ammunition Types: M371 HEAT, M591 HE, M590 APERS
Backblast 0 to 25 m: 100 Bp
          25 to 50 m: 50 Bp
Target Area: Range/ 50; Minimum = 10 m
RANGE
 Minimum      C(9+)  M(12+)  L(14+)  Ex(18+)
   20 m.      200 m. 500 m.  1000 m. 2100 m.
Failure: 11+

M40A4 106 mm RECOLILLESS RIFLE

Nationality: U.S.
Weapon Type: Mounted Recoilless Rifle
Caliber: 106 mm
Length: 340 cm
Weight: 113 kg (Gun only)
        130 kg (Gun and Spotting Rifle)
        88 kg  (M79 Gun Mount)
Type of Fire: Single shot
Rate of Fire: 1 per 2 combat rounds
Feed Device: Single round, breach loaded
Ammunition Types: M344A1 HEAT, M346A1 HEP-T, M581 APERS
Backblast 0 to 25 m: 100 Bp
          25 to 50 m: 50 Bp
Target Area: Range/ 100; Minimum = 10 m
RANGE
 Minimum      C(9+)  M(12+)  L(14+)  Ex(18+)
   50 m.      300 m. 800 m.  1200 m. 7500 m.
Failure: 11+
