M151A2 1/4-ton Morrow Project Light Reconnaissance Jeep

CREW: 1 (Driver) + 1 (Observer/ Gunner) 
CONFIGURATION: 4 x 4
LENGTH: 3.37 m
WIDTH: 1.63 m
HEIGHT (OVERALL): 1.80 m
WEIGHT (EMPTY): 1107 kg
       (LOADED): 1652 kg
MAX LOAD (ROAD): 545 kg
         (CROSS-COUNTRY): 363 kg
MAX. TOWED LOAD (ROAD): 970 kg
                (CROSS-COUNTRY): 680 kg
GROUND CLEARANCE (AXLES): 0.24 m
TURNING RADIUS: 5.63 m
MAX. ROAD SPEED: 90 km/h
MAX. CROSS-COUNTRY SPEED: 30 km/h
FORDING DEPTH: 0.53 m
GRADIENT: 60%
SIDE SLOPE: 40%
VERTICAL OBSTACLE: 
ARMOUR CLASS: 
ARMAMENT: FN MAG 58 7.62 mm MMG, Front Pintle
          Optional FN MAG 58 7.62 mm MMG, Rear Pintle
AMMUNITION: 100/ 900 7.62 mm (Ready/ Stored)
SMOKE LAYING EQUIPMENT: None Normally Installed
EQUIPMENT: See Attached Sheets
NOTES: 
- This vehicle is based on the Israeli Recon M151 Jeep
- Windshield assembly has been completely removed.
- Anti-wire cutting bar is installed on front bumper.
- A roll bar is installed.
- The front pintle is attached in front of the front passenger
  seat.  A second pintle is mounted in the rear passenger area.
- Tires are All-Terrain 10" x 16", with runflat inserts.  Once
  one or more tires are flat, the tires can be run for up to 
  50 km at 30 km/h.  However, the tire may be ruined beyond
  repair.
- The Autonav system is installed below the front passenger seat
  in the old battery compartment, with a read out screen mounted
  on lower portion of the centre of the dash board.
- 2 Spare tires are mounted side by side on the rear of the
  vehicle.  2 23 litre "Jerry Can" style water cans are mounted
  on the 2 rear bumpers in front of the each spare tire. 
- 2 radio sets are installed.  1x AN/PRC-70 radio set w/   & 1x
  AN/PRC-68 radio set w/ OG-174/VRC vehicle adapter.
- 2 antenna mounting brackets are attached just behind the rear
  wheels, to the outside of the vehicle.  Attached to the
  brackets are an MX-6707 Base Matching antenna unit, for the
  AS-1729/VRC Vehicular Antenna.
- With the antenna upright (not recommended), the total height of
  the vehicle is 4.60 m. 
- The suspension of the M151A2 has been improved for a slight
  increase in payload and ride comfort.
- All vehicles start out painted olive drab, and can and should
  be adapted to match local environmental conditions.
- Fusion Engine can be removed and replaced in « an hour, with
  proper tools and crane.
- Payload includes crew, personal gear, BII (Basic Issue Items),
  special kits & equipment and trailer tongue weight.

AMMUNITION:

 M240G 7.62 mm MMG

  ***************** - 
  ***************** - 
  ***************** - 
  ***************** - 
  ***************** - 
  ***************** - 
  ***************** - 
  ***************** - 
  ***************** - 
  ***************** --- 

     AP, AP, AP, AP, API-T, API-T

 Short Burst = 6 rds, Medium = 12 rds, Long = 18 rds

 Armbrust 300

  * - * ---