LAV-25 F

CREW: 3 (Driver, Commander & Gunner) + 3 Passengers
CONFIGURATION: 8 x 8
LENGTH: 6.39 m
WIDTH: 2.50 m
HEIGHT (TURRET): 2.69 m
       (HULL): 1.98 m
WEIGHT (EMPTY): 11 099 kg
       (LOADED): 12 882 kg
CARGO CAPACITY: 2000 kg
MAX. TOWED WEIGHT: 2000 kg
GROUND CLEARANCE: 0.50 m
TURNING RADIUS: 12.00 m
MAX. ROAD SPEED: 101.00 km/h
MAX. CROSS-COUNTRY SPEED: 30.00 km/h
MAX. WATER SPEED: 10.50 km/h
FORDING DEPTH: Amphibious
GRADIENT: 70%
SIDE SLOPE: 40%
VERTICAL OBSTACLE: 0.50 m
TRENCH: 2.06 m
ARMOUR CLASS: 110 all around
ARMAMENT: M242 25 mm Chain Gun, Gyro-Stabilized, Main 
          M240C 7.62 mm Machine Gun, Gyro-Stabilized, Co-Axial
          M240D 7.62 mm Machine Gun, Pintle, Anti-Aircraft
MAXIMUM RATE OF TURRET, POWER TRAVERSE: 25 / second
MAXIMUM RATE OF TURRET, POWER ELEVATION: 25 / second
MAIN & CO-AXIAL GUN ELEVATION/ DEPRESSION: +60 / -10 
TURRET TRAVERSE: 360 
AMMUNITION: 210/ 1050 25 mm (Ready/ Stored), Main
            400/ 1800 7.62 mm, Co-Axial
            200/ 0 7.62 mm, Anti-Aircraft
            4 Anti-Personal, 4 Smoke/ 16 AP, 16 Smoke
SMOKE LAYING EQUIPMENT: 2 x 4 Tube M257 Smoke Launcher
EQUIPMENT: See Attached Sheets
NOTES: 
- The turret is a 2 man turret with Anti-Aircraft MMG mounted to
  the Commanders hatch area.
- Turret traverse can be by Commander or Gunner.
- Winch (Max 9072 kg Tow Limit, 45 m x 12.7 mm Tow Cable).  
- Vehicle is NBCW Proof and Amphibious.
- Tires are 11.00" x 16" Tubeless Tires, with Hutchison Run Flat
  Insert, which are good for 50 Kms once flat.
- Fusion Engine can be removed and replaced in 1 hour, with
  proper tools and crane.

AMMUNITION:

 M242 25 mm Chain Gun

  **************************************************** -  
  **************************************************** -  
  **************************************************** -  
  **************************************************** -  
  **************************************************** -  
  **************************************************** ---  

     APDS-T, APDS-T, APDS-T, HEI-T

 Short Burst = 4 rds, Medium = 8 rds, Long = 12 rds.

 M240C 7.62 mm Co-Axial Machine Gun

  ****************************************************************** - 
  ****************************************************************** - 
  ****************************************************************** - 
  ****************************************************************** - 
  ****************************************************************** - 
  ********************************* --- 

     AP, AP, AP, AP, API-T, API-T

 Short Burst = 6 rds, Medium = 12 rds, Long = 18 rds

 M240D 7.62 mm Anti-Aircraft Machine Gun

  ********************************* --- 

     AP, AP, AP, AP, API-T, API-T

 Short Burst = 6 rds, Medium = 12 rds, Long = 18 rds

 M257 66 mm Smoke/ Anti-Personnel Grenade Launchers

  Left      Right

  SA/AS -    SA/AS -
  SA/AS -    SA/AS -
  SA/AS -    SA/AS -
  SA/AS -    SA/AS -
  SA/AS -    SA/AS ---

     A = Anti-Personal  S = Smoke

 Fired in volleys of 4 or 8 at a time.
 When firing mark off one side of the slash.

 Armbrust 300

  * - * - * - * ---