M1043A1/ M1044A1 HMMWV Armament Carrier w/ Supplemental Armour

CREW: 1 (Driver) + 3 Passengers (1 passenger acts as gunner)
CONFIGURATION: 4 x 4
LENGTH (M1043A1): 4.57 m
       (M1044A1): 4.70 m 
WIDTH: 2.15 m
HEIGHT (W/O ARMAMENT): 1.37 m
       (W/ ARMAMENT): 1.83 m
WEIGHT (M1043A1; EMPTY): 2679 kg
       (M1044A1; EMPTY): 2737 kg
       (M1043A1; LOADED): 3896 kg
       (M1044A1; LOADED): 3896 kg
PAYLOAD (M1043A1): 1217 kg
        (M1044A1): 1159 kg
MAX. TOWED WEIGHT: 1905 kg
GROUND CLEARANCE (AXLES): 0.41 m
                 (CHASSIS): 0.61 m
TURNING RADIUS: 7.32 m
MAX. ROAD SPEED: 105.00 km/h
AVERAGE ROAD SPEED: 50.00 km/h
MAX. CROSS-COUNTRY SPEED: 60.00 km/h
ACCELERATION (0 - 48 km/h): 7 seconds
             (0 - 80 km/h): 20 seconds
FORDING DEPTH (W/0 PREPARATION): 0.76 m
              (W/ PREPARATION): 1.50 m
GRADIENT: 60%
SIDE SLOPE: 40%
VERTICAL OBSTACLE: 0.56 m
ARMOUR CLASS (FRONT): 12 (FRONT WINDSHIELD): 4 (REAR): 12
             (SIDES): 12 (SIDE WINDOWS): 4 (TOP): 7 (BOTTOM): 7
WINDOW HIT: 9+ (Front and Sides)
ARMAMENT: M2HB .50 Calibre Heavy Machine Gun or 
          M240G 7.62 mm Medium Machine Gun or
          Mk 19 Mod 3 40 mm Grenade Launcher
ARMAMENT TRAVERSE: 360ø
AMMUNITION: 105/ 735 .50 cal (Ready/ Stored) or
            100/ 900 7.62 mm or
            50/ 250 40 mm High Velocity
EQUIPMENT: See Attached Sheets
NOTES: 
- The armament is mounted to a pintle mount above gunners
  hatch area (in between the drivers seat and front passenger
  seat.
- A1 improvements, higher cargo payload, rear springs, spring
  seats, frame crossmembers and shocks were modified.
- Winch (Max 2724 kg Tow Limit, 30 m x 9.5 mm Tow Cable), which
  is only mounted on the M1044A1.
- Tires are Goodyear 37x12.5 R16.5, with runflat inserts.
  Once one or more tires are flat, the tires can be run for up to
  50 km at 30 km/h.  However, the tire may be ruined beyond
  repair.
- Fusion Engine can be removed and replaced in 1/2 an hour, with
  proper tools and crane.
- Payload includes crew, personal gear, BII (Basic Issue Items),
  special kits & equipment and trailer tongue weight.

AMMUNITION:

 M2HB .50 cal HMG

  ************ -
  ************ -
  ************ -
  ************ -
  ************ -
  ************ -
  ************ -
  ************ ---

 Short Burst = 10 rds, Medium = 20 rds, Long = 30 rds.

Or

 M240G 7.62 mm MMG

  ***************** - 
  ***************** - 
  ***************** - 
  ***************** - 
  ***************** - 
  ***************** - 
  ***************** - 
  ***************** - 
  ***************** - 
  ***************** --- 

     AP, AP, AP, AP, API-T, API-T

 Short Burst = 6 rds, Medium = 12 rds, Long = 18 rds

Or

 Mk 19 Mod 3 40 mm GL

  HHW, HHW, HHW, HHW, HHW, HHW, HHW, HHW, HHW, HHW, HHW, HHW,
  HHW, HHW, HHW, HH -

  HHW, HHW, HHW, HHW, HHW, HHW, HHW, HHW, HHW, HHW, HHW, HHW,
  HHW, HHW, HHW, HH -

  HHW, HHW, HHW, HHW, HHW, HHW, HHW, HHW, HHW, HHW, HHW, HHW,
  HHW, HHW, HHW, HH -

  HHW, HHW, HHW, HHW, HHW, HHW, HHW, HHW, HHW, HHW, HHW, HHW,
  HHW, HHW, HHW, HH -

  HHW, HHW, HHW, HHW, HHW, HHW, HHW, HHW, HHW, HHW, HHW, HHW,
  HHW, HHW, HHW, HH -

  HHW, HHW, HHW, HHW, HHW, HHW, HHW, HHW, HHW, HHW, HHW, HHW,
  HHW, HHW, HHW, HH ---

 H = High Explosive Dual Purpose  W = White Phosphorus

 Short Burst = 3 rds, Medium = 6 rds, Long = 9 rds

 Armbrust 300

  * - * - * - * ---