COMMANDO V-150 SF AMBULANCE

CREW: 3 (Driver, 2 Medics) + 4 Ambulatory or 2 Litter Patients or
      combination of litter and ambulatory patients
CONFIGURATION: 4 x 4
LENGTH: 6.14 m
WIDTH: 2.26 m
HEIGHT: 2.31 m
WEIGHT (EMPTY): 8054 kg
       (LOADED): 9072 kg
CARGO CAPACITY: 2000 kg
MAX. TOWED WEIGHT: 2000 kg
GROUND CLEARANCE (AXLES): 0.38 m
                 (HULL): 0.65 m
TURNING RADIUS: 8.50 m
MAX. ROAD SPEED: 88.50 km/h
MAX. CROSS-COUNTRY SPEED: 30.00 km/h
MAX. WATER SPEED: 5.00 km/h
FORDING DEPTH: Amphibious
GRADIENT: 60%
SIDE SLOPE: 30%
VERTICAL OBSTACLE: 0.91 m
TRENCH: 0.5 m
ARMOUR CLASS: 100 all around
ARMAMENT: None
AMMUNITION: 4 Anti-Personal, 4 Smoke/ 12 AP, 12 Smoke
SMOKE LAYING EQUIPMENT: 2 x 4 Tube M257 Smoke Launcher
EQUIPMENT: See Attached Sheets
NOTES: 
- Vehicle is the same as the Command and Control vehicle from the
  outside with the exception of, double hinged side doors on both
  sides of the vehicle, where normally the single hinged doors
  are.
- Patients are loaded through the side double hinged doors.  The
  roof area has no provision for a roof mounted hatch or weapons
  station. 
- Full vehicle air conditioning is provided for patient comfort.
- Winch (Max 4536 kg Tow Limit, 48.76 m x 9.5 mm Tow Cable).  
- Vehicle is NBCW Proof and Amphibious.
- Tires are 14.50" x 21" Tubeless Tires, with Hutchinson Run Flat
  Insert which are good for 50 Kms once flat.
- Fusion Engine can be removed and replaced in 1 hour, with
  proper tools and crane.

AMMUNITION:

 M257 66 mm Smoke/ Anti-Personnel Grenade Launchers

  Left       Right

  SA/AS -    SA/AS -
  SA/AS -    SA/AS -
  SA/AS -    SA/AS -
  SA/AS -    SA/AS ---

  A = Anti-Personal   S = Smoke

 Fired in volleys of 4 or 8 at a time.
 When firing mark off one side of the slash.

 Armbrust 300

 * - * - * - * ---