M67 90 mm RECOILLESS RIFLE MUNITIONS

M371A1 HEAT

Type: High Explosive Anti-Tank
Weight (Complete): 4.20 kg
       (Projectile): 3.06 kg
Range (Minimum): 20 m
      (Effective): 250 m
      (Maximum): 400 m
Burst Radius: 20 m
Anti-Armour Class: D
Penetration: n/a (8 per fragment)
DPW: 1821
Packaging: 1 round per fibre tube, 1 tubes to a wooden case.
Packaging Weight: 13.39 kg
NOTES: Primarily for use against armour with vertical armour and
is more effective against "sandwich" or "honey-combed" armour.
The conical shape of the filler is maintained by a copper cone
which forms a slug when the filler is exploded. This slug may or
may not follow the explosive jet through the armour.

M590 (XM590E1) APERS

Type: Antipersonnel
Weight (Complete): 3.08 kg
       (Projectile): 1.80 kg
Range (Minimum): 0 m
      (Effective): 250 m
      (Maximum): 400 m
Burst Radius: A cone up to 250 m long x up to 35 m wide
Anti-Armour Class: n/a
Penetration: n/a (6 per flechette) roll 1d100 to see how many hit
DPW: 28
Packaging: 1 round per fibre tube, 6 containers to a wirebound
           box.
Packaging Weight: 26.33 kg
NOTE: Designed for antipersonnel purposes only. The projectile
contains 2400 flechettes (fin stabilized fragments of steel). The
flechettes are dispersed and are projected forward in an 8o cone
by the rotational force and velocity of the projectile.  The fuze
is set to functions at the muzzle.  The cone of flechettes at the
50 m point; 7 m wide/ high, at the 100 m point; 14 m wide/ high,
at the 150 m point; 21 m wide/ high; at the 200 m point; 28 m
wide/ high; at the 250 m point; 35 m wide/ high.