LAV-25(MC)A1 F

CREW: 3 (Driver, Commander & Gunner/ Loader)
CONFIGURATION: 8 x 8
LENGTH: 6.39 m
WIDTH: 2.50 m
HEIGHT (TURRET): 2.69 m
       (HULL): 1.98 m
WEIGHT (EMPTY): 11 199 kg
       (LOADED): 13 156 kg
CARGO CAPACITY: 2000 kg
MAX. TOWED WEIGHT: 2000 kg
GROUND CLEARANCE: 0.50 m
TURNING RADIUS: 12.00 m
MAX. ROAD SPEED: 101.00 km/h
MAX. CROSS-COUNTRY SPEED: 30.00 km/h
MAX. WATER SPEED: 10.50 km/h
FORDING DEPTH: Amphibious
GRADIENT: 70%
SIDE SLOPE: 40%
VERTICAL OBSTACLE: 0.50 m
TRENCH: 2.06 m
ARMOUR CLASS: 110 all around
ARMAMENT: M242 25 mm Chain Gun, Gyro-Stabilized, Main 
          M240C 7.62 mm Machine Gun, Gyro-Stabilized, Co-Axial
          Twin TOW-II ATGW Launchers, Right Side of turret
          M240D 7.62 mm Machine Gun, Pintle, Anti-Aircraft
MAXIMUM RATE OF TURRET, POWER TRAVERSE: 25ø/ second
MAXIMUM RATE OF TURRET, POWER ELEVATION: 25ø/ second
MAIN & CO-AXIAL GUN ELEVATION/ DEPRESSION: +60ø/ -10ø
TOW LAUNCHER ELEVATION/ DEPRESSION: +30ø/ -20ø
TURRET TRAVERSE: 360ø
AMMUNITION: 210/ 1470 25 mm (Ready/ Stored), Main
            400/ 2200 7.62 mm, Co-Axial
            2/ 4 TOW, Right Side of Turret
            200/ 0 7.62 mm, Anti-Aircraft
            4 Anti-Personal, 4 Smoke/ 16 AP, 16 Smoke
SMOKE LAYING EQUIPMENT: 2 x 4 Tube M257 Smoke Launcher
EQUIPMENT: See Attached Sheets
NOTES:
- Same as LAV-25(MC) F, but with a TOW ATGW launcher mounted to
  the right side of the turret.
- TOW (Tube-launched, Optically-guided, Wire-tracked)
- The launcher can fire any of the TOW missile variants, BGM-71A
  Basic TOW, BGM-71B Extended Range TOW (ER-TOW), BGM-71C
  Improved TOW (I-TOW) or BGM-71D TOW 2, BGM-71E TOW 2A or
  BGM-71F TOW 2B.
- Once the vehicle has stopped it takes only 15 seconds for the
  launcher to be elevated and the target engaged.
- Time from first-round impact to second-round triggering with a
  12.5ø target separation is 4.25 seconds.
- When travelling, the system is retracted to the right side of
  the turret.
- To reload launcher(s), the turret is traversed to the right.
  Where the loader opens the armoured roof hatch on the rear
  deck.  Reaches out and replaces the expended TOW canisters with
  fresh rounds.
- The turret is a 2 man turret with Anti-Aircraft MMG mounted to
  the Commanders hatch area.
- Turret traverse can be by Commander or Gunner.
- Winch (Max 9072 kg Tow Limit, 45 m x 12.7 mm Tow Cable).  
- Vehicle is NBCW Proof and Amphibious.
- Tires are 11.00" x 16" Tubeless Tires, with Hutchison Run Flat
  Insert, which are good for 50 Kms once flat.
- Fusion Engine can be removed and replaced in 1 hour, with
  proper tools and crane.

AMMUNITION:

 BGM-71A Basic TOW or Any Of The Variants

  * * - * * - * * --- 

 M242 25 mm Chain Gun

  **************************************************** -  
  **************************************************** -  
  **************************************************** -  
  **************************************************** -  
  **************************************************** -  
  **************************************************** -  
  **************************************************** -  
  **************************************************** -  
  **************************************************** ---  

     APDS-T, APDS-T, APDS-T, HEI-T

 Short Burst = 4 rds, Medium = 8 rds, Long = 12 rds.

 M240C 7.62 mm Co-Axial Machine Gun

  ****************************************************************** - 
  ****************************************************************** - 
  ****************************************************************** - 
  ****************************************************************** - 
  ****************************************************************** - 
  ****************************************************************** - 
  ********************************* --- 

     AP, AP, AP, AP, API-T, API-T

 Short Burst = 6 rds, Medium = 12 rds, Long = 18 rds

 M240D 7.62 mm Anti-Aircraft Machine Gun

  ********************************* --- 

     AP, AP, AP, AP, API-T, API-T

 Short Burst = 6 rds, Medium = 12 rds, Long = 18 rds

 M257 66 mm Smoke/ Anti-Personnel Grenade Launchers

  Left      Right

  SA/AS -    SA/AS -
  SA/AS -    SA/AS -
  SA/AS -    SA/AS -
  SA/AS -    SA/AS -
  SA/AS -    SA/AS ---

     A = Anti-Personal  S = Smoke

 Fired in volleys of 4 or 8 at a time.
 When firing mark off one side of the slash.

 Armbrust 300

  * - * - * - * ---