ARMORED ENGINEER VEHICLES

M728 COMBAT ENGINEER VEHICLE (CEV)

Crew: 4 (Commander, Driver, Gunner & Loader)
Weight (Empty): 50439 kg
       (Loaded): 53200 kg
Length (With Boom Erected): 9.30 m
       (With Blade and Boom in Travelling Position): 8.91 m
Width (Including Blade): 3.70 m
      (Hull): 3.63 m
Height (Travelling): 3.20 m
       (Lowest Operable): 3.26 m
Ground Clearance: 0.38 m
Max Road Speed: 48 kmph
Fuel Capacity: 1420 Litres (Diesel) 
Max Range: 450 km
Gradient: 60%
Side Slope: 40%
Vertical Obstacle: 0.76 m
Turn Radius: 9.30 m
Fording Depth: 1.22 m
             (With Kit): 2.44 m
Trench: 2.51 m
Armour Value (Hull): F: 860 (400); R: 100; S: 200; T: 140; B: 160
             (Turret): F: 1000 (350); S: 450 (300); T: 140
Armament: 1 x 165 mm Demolition Gun
          1 x M219 or M240 7.62 mm Coaxial
          1 x M85 .50 cal HMG
          2 x 6 Smoke Dischargers
Ammunition: 30 rds 165 mm
            3600 rds 7.62 mm
            600 rds .50 cal
Note: A Frame is pivoted each side of turret and has a maximum
lifting capacity of 15876 kg with two-speed winch and 61 m of 19
mm thick cable.