M100 Trailer, Amphibious, Cargo: 1/4 ton, 2 Wheel

Weight (Empty): 256 kg
       (Loaded; Road): 596 kg
       (Loaded; Cross-Country): 483 kg
Max Load (Road): 340 kg
         (Cross-Country): 227 kg
Length (Overall): 2.68 m
       (Inside Body): 1.83 m
Width (Overall): 1.47 m
      (Inside Body): 0.97 m
Height: 1.07 m
Ground Clearance: 0.35 m
Depth (Inside Body): 0.46 m
Coupling Height: 0.69 m
Tires: 7.00" x 16"
Note: The M100 is a single-axle trailer.  The all-welded body,
bolted to the M115 chassis, is watertight and will float with a
load of 227 kg.  Two drain holes are provided in the floor of the
trailer, which has a support leg and a canvas cover is provided
to cover the cargo area and when not required and when not
required this is stowed in a metal box mounted on the left front
body panel.