M1035/ M1035A1 HMMWV 2-Litter "Soft-Top" Ambulance

CREW: 1 (Driver) + 3 Ambulatory or 2 Litter Patients or
      Combination of litter and ambulatory patients.
CONFIGURATION: 4 x 4
LENGTH: 4.57 m
WIDTH: 2.15 m
HEIGHT: 1.75 m
WEIGHT (M1035; EMPTY): 2361 kg
       (M1035A1; EMPTY): 2361 kg
       (M1035; LOADED): 3496 kg
       (M1035A1; LOADED): 3578 kg
PAYLOAD (M1035): 1135 kg
        (M1035A1): 1217 kg
MAX. TOWED WEIGHT: 1500 kg
GROUND CLEARANCE (AXLES): 0.41 m
                 (CHASSIS): 0.61 m
TURNING RADIUS: 7.32 m
MAX. ROAD SPEED: 105.00 km/h
AVERAGE ROAD SPEED: 50 km/h
MAX. CROSS-COUNTRY SPEED: 40.00 km/h
ACCELERATION (0 - 48 km/h): 7 seconds
             (0 - 80 km/h): 20 seconds
FORDING DEPTH (W/0 PREPARATION): 0.76 m
              (W/ PREPARATION): 1.50 m
GRADIENT: 60%
SIDE SLOPE: 40%
VERTICAL OBSTACLE: 0.56 m
ARMOUR CLASS (FRONT): 10 (REAR): 0 (SIDES): 0 (TOP): 0
             (BOTTOM): 7
WINDOW HIT: 9+ (Front)
ARMAMENT: None
ARMAMENT TRAVERSE: None
AMMUNITION: None
EQUIPMENT: See Attached Sheets
NOTES: 
- The vehicles are equipped with no armour and used to
  transport patients from the battlefield.
- Ambulance is provided with a soft top only, which only provides
  protection from the elements.
- A1 Improvements include higher cargo payload, rear springs,
  spring seats, frame crossmembers and shocks were modified.
- Tires are Goodyear 37x12.5 R16.5, with runflat inserts.
  Once one or more tires are flat, the tires can be run for up to
  50 km at 30 km/h.  However, the tire may be ruined beyond
  repair.
- Fusion Engine can be removed and replaced in 1/2 an hour, with
  proper tools and crane.
- Payload includes crew, patients, personal gear, BII (Basic
  Issue Items), special kits & equipment and trailer tongue
  weight.
