COMMANDO V-150 SF

CREW: 3 (Driver, Commander & Gunner) + 1 Passenger
CONFIGURATION: 4 x 4
LENGTH: 6.14 m
WIDTH: 2.26 m
HEIGHT (TURRET): 2.53 m
       (HULL): 1.98 m
WEIGHT (EMPTY): 8981 kg
       (LOADED): 10 106 kg
CARGO CAPACITY: 2000 kg
MAX. TOWED WEIGHT: 2000 kg
GROUND CLEARANCE (AXLES): 0.38 m
                 (HULL): 0.65 m
TURNING RADIUS: 8.50 m
MAX. ROAD SPEED: 88.50 km/h
MAX. CROSS-COUNTRY SPEED: 30.00 km/h
MAX. WATER SPEED: 5.00 km/h
FORDING DEPTH: Amphibious
GRADIENT: 60%
SIDE SLOPE: 30%
VERTICAL OBSTACLE: 0.91 m
TRENCH: 0.5 m
ARMOUR CLASS: 100 all around
ARMAMENT: M2HB .50 cal HMG, Main 
          40 mm Mk 19 Mod. 3 Grenade Launcher, Co-Axial
MAXIMUM RATE OF TURRET, POWER TRAVERSE (FAST): 45ø/ second
                                       (SLOW): 10ø/ second
MAXIMUM RATE OF TURRET, MANUAL ELEVATION: 10ø/ second
MAIN & CO-AXIAL, GUN ELEVATION/ DEPRESSION: +45ø/ -8ø
TURRET TRAVERSE: 360ø
AMMUNITION: 210/ 840 .50 cal (Ready/ Stored)
            100/ 300 40 mm
            4 Anti-Personal, 4 Smoke/ 12 AP, 12 Smoke
SMOKE LAYING EQUIPMENT: 2 x 4 Tube M257 Smoke Launcher
EQUIPMENT: See Attached Sheets
NOTES: 
- The vehicle has a 500 000 candlepower spotlight mounted co-
  axially with the main gun, that will illuminate up to 1.5 kms
  away.  
- The turret is a 1 man turret.
- Winch (Max 4536 kg Tow Limit, 48.76 m x 9.5 mm Tow Cable).  
- Vehicle is NBCW Proof and Amphibious.
- Tires are 14.50" x 21" with Hutchinson Run Flat Insert, Tubeless Tires,
  which are good for 50 Kms once flat.
- Fusion Engine can be removed and replaced in 1 hour, with
  proper tools and crane.

AMMUNITION:

 M2HB HMG .50 cal

     ********************* -  
     ********************* -
     ********************* -
     ********************* -
     ********************* ---

 Short Burst = 10 rds, Medium = 20 rds, Long = 30 rds.

 Mk 19 Mod 3 40 mm Grenade Launcher

     HHW, HHW, HHW, HHW, HHW, HHW, HHW, HHW, HHW, HHW, HHW, HHW, HHW,
     HHW, HHW, HHW, HHW, HHW, HHW, HHW, HHW, HHW, HHW, HHW, HHW, HHW,
     HHW, HHW, HHW, HHW, HHW, HHW, HHW, H -

     HHW, HHW, HHW, HHW, HHW, HHW, HHW, HHW, HHW, HHW, HHW, HHW, HHW,
     HHW, HHW, HHW, HHW, HHW, HHW, HHW, HHW, HHW, HHW, HHW, HHW, HHW,
     HHW, HHW, HHW, HHW, HHW, HHW, HHW, H -
    
     HHW, HHW, HHW, HHW, HHW, HHW, HHW, HHW, HHW, HHW, HHW, HHW, HHW,
     HHW, HHW, HHW, HHW, HHW, HHW, HHW, HHW, HHW, HHW, HHW, HHW, HHW,
     HHW, HHW, HHW, HHW, HHW, HHW, HHW, H -

     HHW, HHW, HHW, HHW, HHW, HHW, HHW, HHW, HHW, HHW, HHW, HHW, HHW,
     HHW, HHW, HHW, HHW, HHW, HHW, HHW, HHW, HHW, HHW, HHW, HHW, HHW,
     HHW, HHW, HHW, HHW, HHW, HHW, HHW, H ---

 H = High Explosive Dual Purpose  W = White Phosphorus

 Short Burst = 3 rds, Medium = 6 rds, Long = 9 rds

 M257 66 mm Smoke/ Anti-Personnel Grenade Launchers

  Left       Right

  SA/AS -    SA/AS -
  SA/AS -    SA/AS -
  SA/AS -    SA/AS -
  SA/AS -    SA/AS ---

  A = Anti-Personal   S = Smoke

 Fired in volleys of 4 or 8 at a time.
 When firing mark off one side of the slash.

 Armbrust 300

 * - * - * - * ---
