M1097/ M1097A1 Heavy HMMWV (HHV) Cargo/ Troop Carrier

CREW: 2 (Driver & Other) + 8 Passengers/ Troops or Cargo
CONFIGURATION: 4 x 4
LENGTH (M1097): 4.57 m
       (M1097A1): 4.70 m
WIDTH: 2.15 m
HEIGHT: 2.60 m
WEIGHT (M1097 EMPTY): 2542 kg
       (M1097A1; EMPTY): 2600 kg
       (M1097; LOADED): 4540 kg
       (M1097A1; LOADED): 4540 kg
PAYLOAD (M1097): 1998 kg
        (M1097A1): 1940 kg
MAX. TOWED WEIGHT: 1905 kg
GROUND CLEARANCE (AXLES): 0.41 m
                 (CHASSIS): 0.61 m
TURNING RADIUS: 7.32 m
MAX. ROAD SPEED: 105.00 km/h
AVERAGE ROAD SPEED: 50 km/h
MAX. CROSS-COUNTRY SPEED: 40.00 km/h
ACCELERATION (0 - 48 km/h): 7 seconds
             (0 - 80 km/h): 20 seconds
FORDING DEPTH (W/0 PREPARATION): 0.76 m
              (W/ PREPARATION): 1.50 m
GRADIENT: 60%
SIDE SLOPE: 40%
VERTICAL OBSTACLE: 0.56 m
ARMOUR CLASS (FRONT): 10 (REAR): 0 (SIDES): 7 (TOP): 7
             (BOTTOM): 7
WINDOW HIT: 9+ (Front and Sides)
ARMAMENT: None normally, but a weapons station can be added
ARMAMENT TRAVERSE: 180ø if installed
AMMUNITION: As Cargo
EQUIPMENT: See Attached Sheets
NOTES: 
- The vehicles are equipped with basic armour and used to
  transport equipment, materials and/or personnel.  Can also be
  configured in to a 4 man crew configuration.
- Improvements include higher cargo payload, rear springs, spring
  seats, frame crossmembers and shocks were modified.
- Winch (Max 2724 kg Tow Limit, 30 m x 9.5 mm Tow Cable), which
  is installed on the M1097A1 model.
- Tires are Goodyear 37x12.5 R16.5, with runflat inserts.
  Once one or more tires are flat, the tires can be run for up to
  50 km at 30 km/h.  However, the tire may be ruined beyond
  repair.
- Fusion Engine can be removed and replaced in 1/2 an hour, with
  proper tools and crane.
- Payload includes crew, personal gear, BII (Basic Issue Items),
  special kits & equipment and trailer tongue weight.