CADILLAC GAGE TEXTRON STINGRAY LIGHT TANK

CREW: 4 (Commander, Driver, Gunner & Loader)
LENGTH (HULL): 6.44 m
       (GUN FORWARD): 9.30 m
       (OF TRACK ON GROUND): 2.31 m
WIDTH: 2.71 m
HEIGHT: 2.55 m
WEIGHT (EMPTY): 19 387 kg
       (LOADED): 21 205 kg
GROUND PRESSURE: 0.72 kg/cm2
GROUND CLEARANCE: 0.46 m
TURNING RADIUS: 9.35 m
MAX. ROAD SPEED: 67 km/h
MAX. ROAD SPEED ON 10% SLOPE: 34 km/h
MAX. ROAD SPEED ON 60% SLOPE: 8 km/h
MAX. CROSS-COUNTRY SPEED: 15-20 km/h
FORDING DEPTH: 1.07 m
GRADIENT: 60%
SIDE SLOPE: 40%
VERTICAL OBSTACLE: 0.76 m
TRENCH: 2.13 m
ARMOUR VALUE (HULL): F: 250 (125); R: 100; S: 100; T: 50; B: 50
             (TURRET): F: 250 (125); S: 100; T: 50
ARMAMENT: L7A3/ M68 105 mm Low Recoil Gun, Main
          M240C 7.62 mm Machine Gun, Co-Axial
          M2HB .50 cal Heavy Machine Gun, Anti-Aircraft
MAXIMUM RATE OF TURRET, POWER TRAVERSE: 35ø/ second (Stabilised)
MAXIMUM RATE OF TURRET, POWER ELEVATION: 8ø/ second (Stabilised)
MAIN & CO-AXIAL, GUN ELEVATION/ DEPRESSION: +20ø/ -7.5ø
TURRET TRAVERSE: 360ø
AMMUNITION: 8/28 rds 105 mm, Main (Ready/ Stored)
            400/2000 rds 7.62 mm, Co-Axial
            105/1050 rds .50 cal, Anti-Aircraft
            4 Anti-Personal, 4 Smoke/ 12 AP, 12 Smoke
SMOKE LAYING EQUIPMENT: 2 x 4 Tube M257 Smoke Launcher
EQUIPMENT: See Attached Sheets
NOTES:
- 8 rounds are stored in the turret, but only 3 are for immediate
  use, stored vertically to the left of the breech.
- The turret is a 3 man turret with Anti-Aircraft HMG mounted to
  the commanders hatch area.
- Turret traverse can be by Commander or Gunner.
- The Commander sits on the right of the turret with the gunner
  below and to his front.  The loader sits on the left side of
  the turret
- The Main gun is stabilized, so it can be laid and fire while
  moving across county. 
- Vehicle is NBC Proof.
- Fusion Engine can be removed and replaced in 1 hour, with
  proper tools and crane.  Engine comes out the top of the engine
  deck.
- There are about 200 shoes per track.   Each shoe lasts
  approximately 700 km, with the entire tracks life expected to
  be 4000 km.
- 6 road wheels per side.
- Turret basket has been enlarged to accommodate the vehicle
  stores. 

AMMUNITION:

 L7A3/ M68 105 mm Low Recoil Gun

  M393 High Explosive Plastic with Tracer

   * - * - * - * - * - * - * - * - * - * - * ---

  M456 High Explosive Anti-Tank with Tracer

   * - * - * - * - * - * - * - * - * - * ---

  M392A2 Armour Piercing Discarding Sabot with Tracer

   * - * - * - * - * - * - * - * --- 

  M494A3 Anti-Personnel (Flechette) with Tracer
 
   * - * - * - * - * - * - * ---

 M240C 7.62 mm Co-Axial Machine Gun

  ****************************************************************** - 
  ****************************************************************** - 
  ****************************************************************** - 
  ****************************************************************** - 
  ****************************************************************** - 
  ****************************************************************** --- 

     AP, AP, AP, AP, API-T, API-T

 Short Burst = 6 rds, Medium = 12 rds, Long = 18 rds

 M2HB HMG .50 cal

  *********** -
  *********** -
  *********** -
  *********** -
  *********** -
  *********** -
  *********** -
  *********** -
  *********** -
  *********** -
  *********** ---

 Short Burst = 10 rds, Medium = 20 rds, Long = 30 rds.

 M257 66 mm Smoke/ Anti-Personnel Grenade Launchers

  Left       Right

  SA/AS -    SA/AS -
  SA/AS -    SA/AS -
  SA/AS -    SA/AS -
  SA/AS -    SA/AS ---

  A = Anti-Personal   S = Smoke

 Fired in volleys of 4 or 8 at a time.
 When firing mark off one side of the slash.

 Armbrust 300

 * - * - * - * ---