M101 & M101A2 Trailer, Cargo: 3/4 ton, 2 Wheel

Weight (Empty): 608 kg
       (Loaded; Road): 1588 kg
       (Loaded; Cross-Country): 1288 kg
Max Load (Road): 1020 kg
         (Cross-Country): 680 kg
Length (Overall): 3.73 m
       (Inside Body): 2.44 m
Width (Overall): 1.87 m
      (Inside Body): 1.83 m
Height (Over Tarpaulin): 2.11 m
Ground Clearance: 0.36 m
Depth (Inside Body): 0.50 m
Coupling Height: 0.69 m
Tires: 9.00" x 16"
Note: The M100 is a single-axle trailer.  Its body is all steel
and is provided with a hinged tailgate, bows and a tarpaulin
cover.  The body is bolted to an M116 chassis.  The drawbar
assembly is attached to the chassis and a retractable pivoted
front support is attached to the drawbar bracket.