COMMANDO LAV-300 F 81 mm MORTAR VEHICLE

CREW: 5 (Driver, Commander & 3 Mortar Men)
CONFIGURATION: 6 x 6
LENGTH: 6.40 m
WIDTH: 2.54 m
HEIGHT: 1.98 m
WEIGHT (EMPTY): 10 918 kg
       (LOADED): 12 418 kg
CARGO CAPACITY: 2000 kg
MAX. TOWED WEIGHT: 2000 kg
GROUND CLEARANCE (AXLES): 0.38 m
                 (HULL): 0.53 m
TURNING RADIUS: 10.00 m
MAX. ROAD SPEED: 92.00 km/h
MAX. CROSS-COUNTRY SPEED: 30.00 km/h
MAX. WATER SPEED: 5.00 km/h
FORDING DEPTH: Amphibious
GRADIENT: 60%
SIDE SLOPE: 30%
VERTICAL OBSTACLE: 0.61 m
TRENCH: 0.5 m
ARMOUR CLASS: 100 all around
ARMAMENT: M29A1 81 mm Mortar, Main 
          M240D 7.62 mm Machine Gun, Pintle, Anti-Aircraft
MORTAR ELEVATION/ DEPRESSION: +85ø/ -42ø
MORTAR TRAVERSE: 360ø
AMMUNITION: -/60 81 mm Mortar Bombs (Ready/ Stored), Main
            200/ 1000 7.62 mm, Anti-Aircraft
            4 Anti-Personal, 4 Smoke/ 12 AP, 12 Smoke
SMOKE LAYING EQUIPMENT: 2 x 4 Tube M257 Smoke Launcher
EQUIPMENT: See Attached Sheets
NOTES: 
- Winch (Max 9072 kg Tow Limit, 45 m x 12.7 mm Tow Cable).  
- Vehicle is NBCW Proof and Amphibious.
- Tires are 14.50" x 21" Tubeless Tires, with Hutchinson Run Flat
  Insert, which are good for 50 Kms once flat.
- Fusion Engine can be removed and replaced in 1 hour, with
  proper tools and crane.
- M29A1 81 mm Mortar can be removed for ground use, ground
  mounting kit provided.

AMMUNITION:

 81 mm M374A2 High Explosive (40 rds)

  * - * - * - * - * - * - * - * - * - * - * - * - * - * - * -
  * - * - * - * - * - * - * - * - * - * - * - * - * - * - * -
  * - * - * - * - * - * - * - * - * - * ---  

 81 mm M375A2 White Phosphorus

  * - * - * - * - * - * - * - * - * - * - * - * - * - * - * ---
 
 81 mm M301A3 Illuminating

  * - * - * - * - * - * - * - * - * - * - * - * - * - * - * ---
  
 M240D 7.62 mm Anti-Aircraft Machine Gun

  ********************************* - 
  ********************************* - 
  ********************************* - 
  ********************************* - 
  ********************************* - 
  ********************************* --- 

     AP, AP, AP, AP, API-T, API-T

 Short Burst = 6 rds, Medium = 12 rds, Long = 18 rds

 M257 66 mm Smoke/ Anti-Personnel Grenade Launchers

  Left       Right

  SA/AS -    SA/AS -
  SA/AS -    SA/AS -
  SA/AS -    SA/AS -
  SA/AS -    SA/AS ---

  A = Anti-Personal  S = Smoke

 Fired in volleys of 4 or 8 at a time.
 When firing mark off one side of the slash.

Armbrust 300

 * - * - * - * ---