M1045/ M1046 HMMWV TOW Missile Carrier w/ Supplemental Armour

CREW: 1 (Driver) + 3 Passengers (1 passenger acts as gunner)
CONFIGURATION: 4 x 4
LENGTH (M1045): 4.57 m
       (M1046): 4.70 m 
WIDTH: 2.15 m
HEIGHT (W/O ARMAMENT): 1.37 m
       (W/ ARMAMENT): 1.83 m
WEIGHT (M1045; EMPTY): 2679 kg
       (M1046, EMPTY): 2737 kg
       (M1045; LOADED): 3814 kg
       (M1046; LOADED): 3814 kg
PAYLOAD (M1045): 1135 kg
        (M1046): 1077 kg
MAX. TOWED WEIGHT: 1500 kg
GROUND CLEARANCE (AXLES): 0.41 m
                 (CHASSIS): 0.61 m
TURNING RADIUS: 7.32 m
MAX. ROAD SPEED: 105.00 km/h
AVERAGE ROAD SPEED: 50.00 km/h
MAX. CROSS-COUNTRY SPEED: 60.00 km/h
ACCELERATION (0 - 48 km/h): 7 seconds
             (0 - 80 km/h): 20 seconds
FORDING DEPTH (W/0 PREPARATION): 0.76 m
              (W/ PREPARATION): 1.50 m
GRADIENT: 60%
SIDE SLOPE: 40%
VERTICAL OBSTACLE: 0.56 m
ARMOUR CLASS (FRONT): 12 (FRONT WINDSHIELD): 4 (REAR): 12
             (SIDES): 12 (SIDE WINDOWS): 4 (TOP): 7 (BOTTOM): 7
WINDOW HIT: 9+ (Front and Sides)
ARMAMENT: M151A2 TOW Missile Launcher
ARMAMENT TRAVERSE: 360ø
ARMAMENT ELEVATION/ DEPRESSION: +20ø/ -10ø
AMMUNITION: 0/ 6 (Ready/ Stored) TOW Missiles
EQUIPMENT: See Attached Sheets
NOTES: 
- The armament is mounted to a pintle mount above gunners
  hatch area (in between the drivers seat and front passenger
  seat.
- TOW (Tube-launched, Optically-guided, Wire-tracked)
- The launcher can fire any of the TOW missile variants, BGM-71A
  Basic TOW, BGM-71B Extended Range TOW (ER-TOW), BGM-71C
  Improved TOW (I-TOW) or BGM-71D TOW 2, BGM-71E TOW 2A or
  BGM-71F TOW 2B.
- Winch (Max 2724 kg Tow Limit, 30 m x 9.5 mm Tow Cable), which
  is only mounted on the M1046.
- Tires are Goodyear 37x12.5 R16.5, with runflat inserts.
  Once one or more tires are flat, the tires can be run for up to
  50 km at 30 km/h.  However, the tire may be ruined beyond
  repair.
- Fusion Engine can be removed and replaced in 1/2 an hour, with
  proper tools and crane.
- Payload includes crew, personal gear, BII (Basic Issue Items),
  special kits & equipment and trailer tongue weight.

AMMUNITION:

 BGM-71A Basic TOW or Any Of The Variants

  * - * - * - * - * - * --- 

 Armbrust 300

  * - * - * - * ---