M107, M107A1 & M107A2 Trailer, Tank: Water, 1 1/2 ton, 2 Wheel 400-
Gallon

Note: M107A1 stats where different are in []

Weight (Empty): 1034 kg
       (Loaded): 2546 kg
Max Load: 1514 liters
Length: 4.32 [4.14] m
Width: 2.27 [2.08] m
Height: 1.91 [1.96] m
Ground Clearance: 0.41 m
Coupling Height: 0.87 m
Tires: 9.00" x 20"
Fording: Complete Submergence
Note: The M107 series is a single-axle trailer, used to
transport, store and distribute drinking water.  The aluminum
tank has a capacity of 1515 liters and has an elliptical cross
section.  The trailer is provided with a hand water pump and a
7.62 m suction hose for filling.  The M107A1 and M107A2 do not
have a support leg, which is only fitted to the M106 trailer.