M106, M106A1 & M106A2 Trailer, Tank: Water, 1 1/2 ton, 2 Wheel 400-
Gallon

Note: M106A1 stats where different are in []

Weight (Empty): 1034 [1070] kg
       (Loaded): 2547 [2583] kg
Max Load: 1514 liters
Length: 4.23 m
Width: 2.36 m
Height: 2.03 m
Ground Clearance: 0.50 m
Coupling Height: 0.87 m
Tires: 11.00" x 20"
Fording: Complete Submergence
Note: The M106 series is a single-axle trailer, used to
transport, store and distribute drinking water.  The aluminum
tank has a capacity of 1515 liters and has an elliptical cross
section.  The trailer is provided with a hand water pump and a
7.62 m suction hose for filling.  The M106A1 and M106A2 do not
have a support leg, which is only fitted to the M106 trailer.