M104, M104A1 & M104A2 Trailer, Cargo: 3/4 ton, 2 Wheel

Note: M104A1 stats where different are in []

Weight (Empty): 1089 [1238] kg
       (Loaded; Road): 3583 [3733] kg
       (Loaded; Cross-Country): 2449 [2599] kg
Max Load (Road): 2495 kg
         (Cross-Country): 1360 kg
Length (Overall): 4.20 m
       (Inside Body): 2.79 m
Width (Overall): 2.11 m
      (Inside Body): 1.88 m
Height (Over Tarpaulin): 2.52 m
Ground Clearance: 0.49 m
Depth (Inside Body): 0.50 m
Coupling Height: 0.87 m
Tires: 11.00" x 20"
Note: The M104 series is a single-axle trailer.  Its body is
welded plate construction with the wheel housing integral with
the body.  The body has front and rear tailgates, hinged at the
floor line and latched in the closed position by hooks. The M104
is bolted to the m102 chassis.  The M104A2 is identical to the
M104 except that it does not have a hinged tailgate.