M416 & M416A1 Trailer, Cargo: 1/4 ton, 2 Wheel

Weight (Empty): 258 kg
       (Loaded; Road): 599 kg
       (Loaded; Cross-Country): 485 kg
Max Load (Road): 340 kg
         (Cross-Country): 227 kg
Length (Overall): 2.75 m
       (Inside Body): 2.44 m
Width (Overall): 1.54 m
      (Inside Body): 1.04 m
Height: 1.07 m
Ground Clearance: 0.35 m
Depth (Inside Body): 0.28 m
Coupling Height: 0.58 m or 0.66 m
Tires: 7.00" x 16"
Note: The M416 is a single-axle trailer.  The all-welded body,
bolted to the M569 chassis, is watertight and will float with a
load of 227 kg.  Two drain holes are provided in the floor of the
trailer, which has a support leg and a tarpaulin cover.