EXPLOSIVES

M2 Demolition Charge

Weight: 1.13 kg
Relative Effectiveness: 0.93
Packaging: 8 blocks to a haversack, 2 haversacks per wooden crate
Packaging Weight: 25.85 kg
DPW: 1210

M3 Demolition Charge

Weight: 1.02 kg
Relative Effectiveness: 1.00
Packaging: 8 blocks to a haversack, 2 haversacks per wooden crate
Packaging Weight: 25.50 kg
DPW: 1300

M5A1 Demolition Charge

Weight: 1.13 kg
Relative Effectiveness: 1.00
Packaging: 24 blocks per wooden crate
Packaging Weight: 25.40 kg
DPW: 1300

M112 Demolition Charge (C-4 Plastic)

Weight: 0.57 kg
Relative Effectiveness: 1.00
Packaging: 30 blocks per wooden crate
Packaging Weight: 21.77 kg
DPW: 1300

M118 Demolition Charge

Weight: 0.91 kg
Relative Effectiveness: 1.24
Packaging: 20 plastic bags per wooden crate
Packaging Weight: 23.60 kg
DPW: 1500
NOTE: The explosive is in a sheet that can be contoured to the
object to be demolished.  4 sheets are packed per plastic bag.

1/2-pound TNT demolition Charge

Weight: 0.23 kg
Relative Effectiveness: 0.75
Packaging: 30 per wooden crate
Packaging Weight: 19.34 kg
DPW: 500
NOTE: These are rectangular blocks of TNT.

1-pound TNT Demolition Charge

Weight: 0.45 kg
Relative Effectiveness: 0.75
Packaging: 30 per wooden crate
Packaging Weight: 21 kg
DPW: 1000
NOTE: These are rectangular blocks of TNT.

M1 Military Dynamite

Weight: 0.23 kg
Relative Effectiveness: 0.62
Packaging: 50 to a plastic bag, 1 plastic bag per wooden crate
Packaging Weight: 15 kg
DPW: 1100

M183 Satchel Charge

Weight: 9 kg
Relative Effectiveness: 16
Packaging: 2 satchel charges per wooden crate
Packaging Weight: 25.85 kg
DPW: 20800
NOTE: 10 blocks of M112 per satchel charge.

M186 Primercord

Weight: 11.34 kg per roll
Length of Roll: 15.24 m
Relative Effectiveness: 1.24 per meter
Packaging: 1 spool per canvas bag, 3 canvas bags per wooden crate
Packaging Weight: 52.10 kg
Blast Radius: 0.5 m
DPW: 10 per meter
NOTE: It can be used for connecting explosive charges so they
detonate simultaneously.  The cord will detonate explosives and can
itself be used as an explosive charge.  Gunfire will detonate
primercord.  The cord detonates at 24000 fps (7317 mps).

40-pound Cratering Charge

Weight: 19.50 kg
Packaging: 1 metal can per wooden crate
Packaging Weight: 23.60 kg
DPW: 3000
NOTE: This is in a water proof metal can.  It is mainly used to
produce craters in roads.  It will produce a crater 0.75 m deep by
1.5 m in diameter.

M3A1 40-pound Shaped Charge

Weight: 13.60 kg
Packaging: 3 per wooden crate
Packaging Weight: 29.50 kg
DPW: 500
NOTE: This is a charge for blasting holes in walls.  It will create
a man sized hole through a wall upto 0.5 m thick.

NITROGLYCERINE

Weight: 0.02 kg
Relative Effectiveness: 1.12
Packaging: Stored in a 118 ml glass or plastic vile
DPW: 100
NOTE: This is a liquid explosive component of dynamite and TNT.  It
is EXTREMELY unstable, and will explode on a roll of 7+ for each CR
it is dropped, bumped, jiggled, shaken or exposed to fire.  It will
automatically explode if the container is broken or punctured.

EXPLOSIVE DETONATORS

M2A1 Detonator

Weight: 0.50 kg
Fuse Delay: 8 seconds
Packaging: 200 per wooden crate
Package Weight: 27.90 kg
NOTE: This is a combination igniter/ fuse/ detonator assembly. 
With the detonator imbedded in the explosive being used the T-ring
is pulled and the fuse is ignited 8 seconds later and the explosive
will detonate.

M1 Timer/ Detonator

Weight: 0.30 kg
Fuse Delay: 10 seconds to 48 hours
Packaging: 150 per wooden crate
Package Weight: 26 kg
NOTE: An adjustable mechanical detonator.  The time delay can be
set from 10 - 60 seconds and from 1 - 10 minutes in 1 minute
intervals and from 1 - 48 hours in 1 hour interval.

M700 Time Fuse

Weight: 0.45 kg per 15 meters
Fuse Delay: 1 second per cm
Packaging: 80 15 m rolls per wooden crate
Package Weight: 29 kg
NOTE: This is a waterproof, plastic covered fuse used to time
explosive charges.  A 15 meter coil burns for 25 minutes.  To
detonate explosives a blasting cap must be crimped on one end. 

M7 Blasting Cap

Weight: 0.004 kg
Packaging: 3600 per wooden crate
Package Weight: 51.50 kg
DPW: 1
NOTE: This cap will detonate explosives.  A fuse must be inserted
into the cap for ignition.

M60 Fuse Igniter

Weight: 0.07 kg
Packaging: 300 per wooden crate
Package Weight: 25.20 kg
NOTE: With this igniter a fuse may be lit underwater.  To use the
igniter, a fuse is placed in the base, the safety pin is removed
and the igniter ring pulled.
